A review on fly ash from coal-fired power plants:

Chemical composition, regulations, and health evidence.

Short Title: Fly-Ash-Review

1. Kristina M. Zierold, PhD

Environmental Health Sciences, University of Alabama at Birmingham, Birmingham, USA

1. Chisom Odoh, PhD

Rehabilitation and Health Services, University of North Texas, Denton, Denton, USA

Corresponding Author:

Kristina M. Zierold, PhD

Fax: (205) 975-6341

Phone: (502) 216-9673

Email: [kzierold@uab.edu](mailto:kzierold@uab.edu)

Word Count without abstract and references: 8,580

Tables/Figures: 1

References: 235

**Abstract**

Throughout the world, coal is responsible for generating approximately 38% of power. Coal ash, a waste product, generated from the combustion of coal, consists of fly ash, bottom ash, boiler slag, and flue gas desulfurization material. Fly ash, which is the main component of coal ash, is comprised of spherical particulate matter with diameters that range from 0.1 µm to >100 µm. Fly ash is predominately composed of silica, aluminum, iron, calcium, and oxygen, but the particles may also contain heavy metals such as arsenic and lead at trace levels. Most nations throughout the world do not consider fly ash a hazardous waste and therefore regulations on its disposal and storage are lacking. Fly ash that is not beneficially reused in products such as concrete, is stored in landfills and surface impoundments. Fugitive dust emissions and leaching of metals into groundwater from landfills and surface impoundments may put people at risk for exposure. There are limited epidemiological studies regarding the health effects of fly ash exposure. In this article, the authors provide an overview of fly ash, its chemical composition, the regulations from nations generating the greatest amount of fly ash, and epidemiological evidence regarding the health impacts associated with exposure to fly ash.

Keywords: Fly ash, coal ash, coal-fired power plants, air pollution, particles

**INTRODUCTION**

Coal is an abundant fossil fuel used for the generation of approximately 38% of the electricity used globally (1). From 2017-2018, the use of coal to produce power increased 3% in the world, but was driven by increased use in China, India, and Southeast Asia. While Asia increased its electricity production from coal, power generated from coal in Europe and the United States decreased over the same year (-2% Europe and -5% United States) (1).

The use of coal for energy production varies throughout the world. In 2016, China, India, and the United States ranked as the top three nations of the world for coal combustion (2). In the United States coal-fired power plants account for approximately 27-30% of electricity generation (3, 4) as compared with China and India, where coal accounts for approximately 72% of the power generated in the nations (5-7).

When coal is burned for energy, coal combustion products (CCPs), often referred to as “coal ash”, are generated. CCPs include fly ash, bottom ash, boiler slag, and flue gas desulfurization material. Baig and Yousaf (2017) reported that for every four tons of coal that is burnt, one ton of coal ash is produced (8). Coal with high ash content will produce more coal ash (9). The composition of coal ash varies based on the geochemical properties of the coal being burned, the mining and preparation methods, the emission control technology used, and the method of burning (10-17). There are four types of coal: anthracite, bituminous, sub-bituminous, and lignite. These coals produce coal ash that is comprised predominately of silicon, aluminum, calcium, and iron and may contain heavy metals, such as arsenic and lead (18-34). The pH of coal ash, which is an important property for leaching of the trace metals, ranges from acidic to alkaline. However, coal ash from bituminous coal contain much less calcium than subbituminous coals, therefore generating ash that is slightly acidic to slightly alkaline on contact with water. Subbituminous coal ash tends to contain a higher concentration of calcium and generates alkaline solutions on contact with water (16, 35).

In 2016, throughout the world, approximately 1.2 billion tonnes of CCPs were produced (36). China, India, Europe and the United States produce the most CCPs. In 2016, China produced over 565 million tonnes, India produced 197 million tonnes, and Europe produced 140 million tonnes (36). According to the U.S. Environmental Protection Agency (EPA), CCPs are one of the largest industrial waste streams in the United States (37). In the United States in 2016, more than 107 million tonnes of coal ash were produced (36, 38)

Coal ash is either beneficially reutilized in products such as concrete and wallboard, or stored in landfills, surface impoundments, or mines. Most power generating facilities store the ash on site (39, 40). Of the total coal ash produced in the world, 64% of coal ash was beneficially used. Harris et al. (2019) reported that Japan had the highest utilization rate (99.3%), followed by Europe (94.3%), Korea (85%), and China (70%) (36).

The coal ash that is not used in products is disposed of in landfills or surface impoundments which may become a potential source of pollution (41-45). In 2010, the EPA reported that “without fugitive dust controls, levels at nearby locations could exceed 35 µg/m3 established as the level of the 24-hour PM2.5 National Ambient Air Quality Standard (US) for fine particulate” (41). Furthermore, the EPA noted that constituents of coal ash such as arsenic have leached at levels of concern from unlined and inadequately clay-lined landfills and surface impoundments (42).

Although some countries like the United States are phasing out the use of coal-fired power plants, other countries like India and Japan are building more coal-fired power plants to meet the supply of power needed for their country (46, 47). Fly ash, which is the CCP that is generated in the greatest quantities, is becoming an increasing environmental threat, as its management is becoming a greater concern among countries’ governing bodies and populations living near coal ash storage facilities.

The purpose of this article is to provide an overview of fly ash including, its chemical composition, regulations that govern fly ash disposal, and the potential health effects from exposure to respirable fly ash and metals found in fly ash.

**METHODS**

Peer- reviewed articles, presentations, and government websites from 1987 to 2019 were assessed using Google Scholar, PUBMED, and web resources. Search keywords included, but were not limited to “coal ash”, “fly ash”, “coal ash regulations”, “coal ash storage” “metals found in fly ash”, “global fly ash,” “groundwater and fly ash,” “leaching behavior of fly ash,” and “coal ash and health.” For additional supportive information, search keywords included “air pollution and health” and “heavy metals and health.” The reference sections of the selected articles were further examined for derivation of relevant articles. The information selected for this review is comprised of web-based articles, government documents, review articles, papers presented at conferences, and full text manuscripts, which were written in English. Overall, 235 references were utilized for this review.

**RESULTS**

1. Fly Ash

Fly ash constitutes the majority of CCPs representing about 40-90% of the total product (48-53). Pulverized fuel combustion has been utilized for over 100 years and most large plants utilize this method. Fly ash is generated when pulverized coal is blown into a combustion chamber. In the combustion chamber, the pulverized coal ignites, generates heat, and produces a molten mineral residue. As heat is extracted by the boiler tubes, flue gases are cooled and the residue hardens and forms an ash. Larger, heavier ash particles fall to the bottom of the combustion chamber. Lighter ash particles remain in the flue gases and are collected in air pollution control devices. These lighter ash particles are termed fly ash (35). Fly ash is a fine silt of spherical powdery particles with diameters that range from 0.1 µm to > 100 µm. Particle sizes of most fly ash from bituminous coal are < 75 µm (16). Fly ash from subbituminous coal tends to be coarser than fly ash from bituminous coal (49). Brown et al. (2011) reported that within the respirable range, the average sphere size ranged from 1.98 µm to 5.64 µm (11). The spherical particles that make up fly ash are grouped into plerospheres and cenospheres. Plerospheres are hollow spheres filled with smaller spheres; whereas empty spheres are termed cenospheres (35). The unique hollow sphere morphology allows for a range of specific gravities of fly ash. Specific gravities range from 1.6-3.1 and pH values can range from 1.2 to 12.5, with the majority of ashes being more alkaline (16, 48, 49, 53-62). Fly ash varies in color, based on the amount of unburned carbon and iron (48, 59). It can be orange to deep red, white to grey, or yellow or black. (48, 49, 60, 63).

Once collected from the air pollution control devices, fly ash is beneficially used in products or as fill in roads or park construction. Countries vary widely on the amount of fly ash that they beneficially utilize. India, China, Canada, and the United Kingdom reutilize 50% or less of generated fly ash; while the United States utilizes approximately 65% (9, 44, 48, 60, 64, 65). Of the reutilized fly ash, the United States uses most of its fly ash (61%) in concrete, concrete products, grout, and in mining applications; China uses most of its fly ash (67%) in cement, bricks, and tiles, India uses most of its fly ash (61%) in cement and reclamation, and the European Union uses most of it fly ash (62%) in reclamation, restoration, and as a concrete addition (59, 64).

Fly ash that is not utilized is predominately stored in landfills or surface impoundments. Due to the chemical composition of fly ash, the size distribution of fly ash, and the mobility of elements from fly ash, concerns have been raised that the fly ash storage methods, particularly older landfills and surface impoundments which are unlined, may harm the environment and impact human health.

1. Chemical Composition of Fly Ash

Fly ash is composed mainly of silica, aluminum, iron, calcium, oxygen and contains many other elements at trace levels (29, 48, 59, 63, 66, 67). Hatori et al., (2010) reported that 80-95% of the sum of oxygen, silica, and aluminum make up the total mass of fly ash particles. Although oxygen, silica, and aluminum, showed homogeneous distributions in the particles that Hatori and researchers studied, they also found that the trace elements were quite different in each particle (29). Some of the trace elements found in fly ash are heavy metals, such as arsenic, cadmium, chromium, and lead (11, 18, 29, 30, 48, 51, 66, 68, 69) and have become an environmental and health concern globally.

Multiple researchers have studied the composition of fly ash and have reported that the concentrations of metals are higher in fly ash than in the parent coal (70-72). Spencer and Drake (1987) assessed fly ash from Iowa, United States, and found that the trace elements of metals existed in concentrations two times greater than metals found in the original coal (70). Bhangare et al (2011) found that in ashes from India, that concentrations of lead, copper, cadmium, zinc, iron, manganese, chromium, nickel, magnesium, lithium, cobalt, mercury, and arsenic were higher in fly ash, compared to bottom ash or coal (71). Yao et al, (2015) reported that trace element levels in Chinese coal may be 4 to 10 times higher than found in the original coal (53). Verma et al (2016) reported concentrations of five metals in coal and in the corresponding fly ash. The concentration of lead in coal was 4 ppm and was found to be 35 ppm in fly ash. The concentration of chromium was 8 ppm in the parent coal and 65 ppm in the fly ash (72).

Understanding the behavior of trace elements during combustion is important in understanding the chemical composition of fly ash. Temperature of the boiler impacts volatilization which effects the distribution of trace elements (16, 68). In understanding the behavior or trace elements, many researchers use the classifications developed by Rudd Meij which details behavior according to their volatility and condensation. Based on the relative enrichment factor which is given in equation 1, Meij created three classifications of trace elements.

(Equation 1)

Class I are nonvolatile elements, Class II are elements that are volatile in the boiler, but condense on the fly ash particles in the electrostatic precipitator (ESP). Class II is divided into three groups with increasing volatility. Finally, Class III represents elements that are very volatile and may not condense on ash at all (27, 33, 68).

Table 1. Classification of Trace Elements.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Description | Relative Enrichment Factor | Examples of Elements | Distribution |
| Class I | Nonvolatile elements | RE ~1 | aluminium, calcium, iron, magnesium | More likely to be in bottom ash or equally distributed in fly ash and bottom ash |
| Class II | Volatile in boiler, condenses in electrostatic precipitator | RE < 0.7 |  |  |
| Class IIc |  |  | chromium, manganese, barium, rubidium |  |
| Class IIb |  |  | beryllium, cobalt, copper, nickel |  |
| Class IIc |  |  | arsenic, cadmium, lead, zinc |  |
| Class III | Very volatile , some do not condense in electrostatic precipitator | RE <<1 | chlorine, fluorine, mercury, selenium | Flue gas, fly ash, but not likely to be in bottom ash |

Elements like chlorine and fluorine are almost totally volatilized in flue gas and do not concentrate in bottom ash. However, as the flue gas cools down, some volatile elements may condense on the surface of the fly ash particles. For example, much higher quantities of arsenic, copper, and selenium, are found in fly ash than are found in bottom ash or boiler slag (39).

Bhangare et al. (2011) assessed thirteen trace elements from five coal-fired power plants in India. The researchers found that chromium, manganese, lead, and iron had RE >1 and that arsenic, mercury, zinc, and lithium had RE<0.7. The remainder of the elements which included cadmium, nickel, cobolt, manganese, and copper had RE that ranged between 0.7 and 1.0, representing the semi-volatile nature of these elements (71).

*Heavy Metals Often Found in Fly Ash*

Heavy metals such as arsenic, lead, chromium, and cadmium are often found in fly ash and may escape as fugitive dust or leachate from landfills and surface impoundments. Although concentrations of trace elements are low, usually in the parts per billion to parts per million range, concern about exposure is apparent in many countries throughout the world (41, 44, 48, 53, 66).

1. *Arsenic (As)*

Inorganic arsenic is one of the most toxic metals found in coal ash and it is a hazardous environmental pollutant. Arsenic concentrations in fly ash range from less than the detection limit to 1000 mg/kg, depending on the parent coal (31, 66, 71, 73-75). The toxicity of As is related to its form, valence state, solubility, the rate of absorption and the rate of elimination. Trivalent arsenic (AsIII) is considered to be more toxic than pentavalent arsenic (AsV) (76-78). The United States Geological Survey (USGS) collected fly ash samples from three coal-fired power plants in the United States. They reported that 89% of arsenic was present as the more oxidized pentavalent arsenic (AsV) whereas only 11% was present as trivalent arsenic (AsIII) (79). Huggins et al. (2007) also found that AsV was present in much greater quantities, than AsIII (80).

Inorganic trivalent and pentavalent compounds are associated with multiple health effects. The International Agency for Cancer Research (IARC) classifies inorganic arsenic as a carcinogen (81). The evidence from drinking-water exposure allows IARC to state that carcinogenicity is related to exposure to AsIII and AsV. However, the evidence from inhaled arsenic mixtures only allows IARC to state that the carcinogenicity is related to inorganic arsenic compounds. Unlike drinking water exposure, IARC states that the evidence for inhalation does not allow a separation of the carcinogenic risk associated with particular arsenic species that occur in these mixtures (81).

In addition to cancer, studies have shown that chronic exposure to arsenic is associated with heart disease (82-85), type 2 diabetes (83, 86-89), impairments in children’s intellectual function (90-92), and respiratory conditions (93-96).

1. *Lead (Pb)*

Lead is a naturally occurring element that is found in the Earth’s crust, therefore it is can be found in the soil, dust, air, and water. Lead is found in parent coals throughout the world. Hence, Pb is also found in fly ash (97-99). Researchers have found Pb concentrations in fly ash that range from less than 1.4 mg/kg to 2,120 mg/kg (31, 71, 74, 75, 100-102). Franus et al. (2015) reported that among the toxic elements in fly ash, Pb and As are found in the greatest amounts (103).

Exposure of children to Pb is of particular concern because their nervous system is still developing. Lead exposure can result in impaired learning, slow growth, behavioral problems, lower IQ and hyperactivity in children (104-109). Chronic Pb exposure can also affect adults and result in health problems like hypertension, hearing problems, poorer kidney function, cognitive impairment, and increased mortality for heart disease (110-114).

Although Pb is most noted for its effects on the central nervous system, IARC has classified inorganic Pb as a probable carcinogen to humans. IARC states that there is limited evidence in humans for the carcinogenicity of inorganic lead compounds and there is inadequate evidence in humans for the carcinogenicity of organic lead compounds. (115)

1. *Chromium (Cr)*

Chromium is a naturally occurring element found in rocks, plants, and soil. It occurs in coal and is released into the air, soil, and water. Chromium exists in three forms, chromium(0), chromium(III), and chromium(VI). It is persistent in the environment, and is of concern because Cr(VI) is a known human carcinogen and certain compounds are highly soluble in water. Cr(III) is less toxic and less soluble than Cr(VI) (116,117).

Chromium is more likely to occur primarily as Cr(III) in most bituminous coals (116, 118-120). There is limited presence of Cr(VI) (121). Researchers have found that, Cr(VI) in coal is reduced in the flue gas by sulfur dioxide (SO2), during the combustion process. It is estimated that the fraction of Cr(VI) in fly ash is less than 5% (118, 121). However, Huggins et al, 1999 reported that some samples of fly ash may contain up to 20% of Cr(VI) (121). Chromium concentrations range in fly ash from 7.82 mg/kg to 651 mg/kg (31, 71, 73-75, 101, 102).

Small amounts of Cr(III) are needed for biological processes in humans, however exposure to Cr(VI) is of great concern. IARC classifies Cr(VI) compounds as known human carcinogens which can cause cancer of the lung, nose, and nasal sinus. There is less evidence for other cancers. (122). Epidemiological studies have reported that Cr(VI) may also be associated with cancer of the stomach, however the results are conflicting (122-125). In addition to cancer, there is some evidence that exposure to Cr(VI) is genotoxic. Lymphocytes of workers exposed to dusts of Cr(VI) compounds showed elevated occurrences of DNA strand breaks, sister chromatid exchange, and micronuclei (126-129).

1. *Cadmium (Cd)*

Cadmium is an element that is also found in the earth’s crust. Although Cd is used in batteries, televisions, and paint pigments, the most significant source of cadmium exposure in humans is cigarette smoke exposure (130). Cadmium is found in coals and hence it is in fly ash. Concentrations of Cd in fly ash range from less than the detection limit to 17 mg/kg (31, 71, 73-75, 101, 102).

Exposure to cadmium may affect several organs in the body. IARC classifies Cd and its compounds as carcinogenic and reports that there is sufficient evidence that Cd is associated with lung, kidney, and prostate cancer (131). Cadmium exposure has been associated with osteoporosis, muscoskeletal pain, kidney failure, and hypertension (132-137).

1. *Mercury (Hg)*

Mercury exists in different forms; as organic, elemental, and inorganic. All these forms are toxic. Humans can be exposed to Hg via food, air pollution, industrial, occupational and agricultural activities (138, 139). Mercury has a low excretion rate; little of it is excreted while the rest is absorbed by different organs in the body (e.g. kidney and liver) to produce neurotoxic and deteriorating effects (138, 140). The effects of Hg on neurobehavioral development in early years have also been reported (140-143). Mercury is found in fly ash with concentrations ranging from less than the detection limit to 2.13mg/kg (71, 74, 75).

1. Regulations Associated with the Storage of Fly Ash

Regulations regarding fly ash disposal vary by country and reflect whether countries consider fly ash as a hazardous waste (16, 36) or another form of waste. In most countries, fly ash is not considered a hazardous waste, thus there are limited rules and regulations that govern its storage and disposal.

1. *Disposal Regulations in the United States*

Prior to 2015, there were very limited regulations on disposal and storage of fly ash in the United States, because it was never considered a “hazardous waste.” In 1978, the Resource Conservation and Recovery Act (RCRA) was enacted by the United States’ Congress, which mandated that the EPA identify and regulate hazardous wastes. When EPA defined “hazardous wastes” under Subtitle C of RCRA, coal ash and five other large waste streams were termed “special wastes” until more research could be conducted on the human health and environmental impact of these wastes. In 1980, the United States’ Congress enacted the Solid Waste Disposal Act Amendments including the Bevill Amendment. The Bevill Amendment exempted “special wastes,” specifically fossil fuel combustion waste, from regulation until additional assessment of risk was conducted. After studying the wastes, EPA determined that coal combustion waste did not belong under Subtitle C of RCRA and was therefore not declared “hazardous.” Since the waste was not hazardous, its disposal falls under Subtitle D of RCRA; which means that it was not regulated by the federal government; instead each state in the United States was to regulate the waste.

Years after the final decision on the classification of coal ash, there were occurrences of large coal ash spills from surface impoundments in Kingston, Tennessee and Eden, New York which led to damage of property and environmental pollution. Collapse of the dike used to contain coal ash by the Tennessee Valley Authority plant at Kingston Tennessee, resulted in spillage of over 4 million cubic meters of coal ash into nearby rivers and surrounding areas. Elevations of various neurotoxic and teratogenic metals and compounds especially methyl mercury were reported in the area (144-146).

Based on studies that reported the possible harmful effects that could result from improper disposal and storage of coal ash, in 2015 the EPA released a Coal Combustion Residuals (CCR) Rule that set requirements for the disposal of coal ash from coal-fired power plants (37). The Coal Combustion Residuals (CCR) Rule was established under the Resource Conservation and Recovery Act (RCRA), Subtitle D. However, although regulations were set forth, coal ash was still not considered a hazardous waste. The CCR rule addressed regulations of ponds and landfills, plant’s location, safety practices, ground water protection, transfer of particles into air as dust, and rules for ash impoundment sites (37). In addition, the rule required facilities to document and make public any information or changes they make regarding the ruling (37). The rule provided a comprehensive and more rigorous design, monitoring, operating, corrective action, closure, and post-closure requirements for CCR landfills and surface impoundments. The CCR rule was applicable to old, new, and existing facilities and did not apply to plants and facilities that were already closed or no longer being used to generate energy. The CCR rule was in existence until July 2018, when the current government of the United States started to roll-back the regulations to allow more flexibility to industry.

1. *Disposal Regulations in India*

Approximately 70-75% of electricity generated in India comes from coal-fired power plants (9, 64, 66, 147). The quality of coal is poor, having a low calorific value and a high ash content (9, 66,147). The use of high ash coal produces fly ash in large quantities and disposal and storage has become a problem, throughout India, although fly ash is not currently considered to be a hazardous waste.

The government of India has attempted to regulate fly ash based on utilization. In 1999, the Ministry of Environment and Forests (MoEF) issued a regulation mandating the need for the reutilization of fly ash. According to the regulation, it was mandatory for existing coal-fired power plants and new coal-fired power plants to utilize 100% of the generated fly ash in a specified time period. New coal-fired power plants were required to use 100% of fly ash within nine years of start-up. Old plants were required to achieve 100% utilization within 15 years from the MoEF regulation (9). This MoEF regulation also mandated that fly ash be provided free of charge to potential users until 2009. Utilization rates throughout India increased, but could not keep up with the amount of ash that was generated. One-hundred percent re-utilization has never been achieved. In response to not being able to meet the 100% utilization rate, the Ministry of Environment, Forests and Climate Change (MoEFCC) mandated that in addition to being required to utilize 100% of fly ash, the power plants were required to pay for the transportation of fly ash to sites within a radius of 300 kilometers of road construction projects and programs of the government involving construction of buildings, roads, dams, and embankments. Furthermore the MoEFCC granted permission for fly ash to be used in agriculture. Plants are required to give free fly ash within a 300 kilometer radius (64).

1. *Disposal Regulations in China*

Accompanying the rapid economic and population growth in China, comes with a high energy demand and enormous production of CCPs (62, 148). In China, the increased production of fly ash alongside with its environmental impact has necessitated an increase in the utilization of fly ash, as a regulatory measure (149, 150).China does not consider fly ash a hazardous waste, instead the country classifies it as a solid industrial waste (16, 62). In China, two agencies are responsible for coal ash management: the National Development and Reform Commission (NDRC) and the Ministry of Environmental Protection (MEP). NDRC is responsible for overseeing fly ash reutilization and MEP is responsible for ensuring that fly ash does not pollute the environment (16). Subsequently, a series of standards, regulations, and requirements were introduced including the Management Measure for Comprehensive Utilization of Fly Ash, which entails special measures regarding the utilization of fly ash (62, 150).

He et al. (2012) reported that the Law of the People’s Republic of China on the Prevention and Control of Environmental Pollution by Solid Waste further divides solid wastes into class I and class II. Fly ash is marked as a class II solid waste, and therefore the fly ash that is not reutilized can be placed in storage facilities. For ash that is not reutilized the Standard for Pollution Control on the Storage and Disposal Site for General Industrial Solid Wastes applies (16, 62). This standard provides directions for where the waste should be stored and measures to prevent fugitive dust and leakage from the storage sites (62) However, according to investigations by Greenpeace, the majority of coal ash storage sites did not meet minimal standards. For example, one of the fly ash storage sites was found to be within 500 meters of residential homes, which violates one of the regulations in the Standards for Pollution Control on the Storage and Disposal of Sites for General Solid Waste (151).

Although there are other regulations that can be applied to fly ash storage facilities, most are voluntary. He et al (2012) claims that the standards are ineffective in constraining coal-fired power plants (62).

1. Exposure Pathways to Humans
2. *Inhalation*

Since fly ash contains particles in the respirable range, unused fly ash stored in landfills and surface impoundments can lead to air pollution and resulting health conditions associated with exposure to particulate matter (41, 60, 62). Poorly managed storage facilities that hold dry ash are susceptible to winds that create fugitive dust that can impact communities living near the storage facilities. The smaller particles, those with diameters less than 10 µm when inhaled, can penetrate deep into the lungs leading to inflammation of cells and irritation of the mucous membrane of the respiratory tract leading to respiratory and cardiovascular conditions associated with exposure to particulate matter (152-155).

In addition to respiratory and cardiovascular conditions, chronic exposure to particulate matter has been found to cause chronic inflammation and elevated levels of cytokines in the body and brain increasing the risk for diseases related to the central nervous system (CNS) (156, 157). Researchers have shown that metals can enter the brain through several pathways, including the nasal olfactory pathway and by crossing red blood cell membranes.

Calderon-Garciduenas et al.’s (2007) research showed that particulate matter <2.5 µm (PM2.5) is capable of passing through the nasal olfactory pathway into the circulatory system and brain. Researchers hypothesize that the large ratio of surface to volume allows the particles to penetrate cell membranes and pass through the lung tissue and the blood-brain barrier. Particulate matter that crosses the blood-brain barrier, introduces the components in the particles to the brain and bloodstream. Researchers call this the Trojan Horse Effect (156, 157). This effect may potentially allow concentrations of metals from fly ash access to the brain, producing CNS disease.

1. *Ingestion*

In addition to the threat of air pollution from fugitive dust, long term storage of fly ash in surface impoundments may impact the environment and human health. Water infiltration, leaky storage sites, and unlined sites may result in metals and other elements leaching from fly ash into the environment. The leaching of elements from fly ash has the potential to impact groundwater and surface water, which is a major concern for humans, especially populations that rely on well water as their drinking source.

Elements that leach from fly ash particles tend to be positioned on the surface of the particle, where there is a gradient of element concentrations (158, 159). Although the surface layer is only microns in thickness, it contains a significant amount of leachable elements (158). The surface layer of fly ash particles is more likely to contain trace elements such as As, boron (B), Hg, Cr, selenium (Se), Cd, copper (Cu), molybdenum (Mo), antimony (Sb), vanadium (V) and zinc (Zn). Elements that tend to distribute throughout the core of the particle, such as manganese (Mn) and Pb, are not directly exposed to leaching (160). The releases of elements distributed throughout the core are controlled by diffusion and are dependent on the dissolution rates of the surface layers (159).

Leaching behavior of trace metals from fly ash has been well-studied. The ability of elements to leach from fly ash depends on properties including pH of the fly ash, pH of the water, amount of lime present in the fly ash, mineralogy of other compounds, particle size, time, reduction-oxidation conditions, liquid to solid ratio, and temperature (45, 74, 100, 102, 147, 161-166). However, it is reported that pH is the greatest factor for mobility of trace metals in water, and that the greatest leaching of metals occurs under an acidic environment (45, 162, 165, 167-170). Since different coals contain different trace elements and have different pHs, leaching of metals from fly ash can vary widely (74).

Leaching of As, which is oxyanionic and positioned on the surface of the fly ash particle, is a major threat from disposal sites because it is mobile throughout a range of pH values (171). Van der Hoek et al. (1994) reported that releases from acidic fly ash increase with pH, whereas in alkaline fly ash this trend is reversed (172). In India, where ash content in coal is high, Kapoor and Christian (2016) reported that fluorine (F), As, magnesium (Mg) and Zn showed solubility with water and was leached in higher concentration at acidic pH and higher temperature (173). Researchers have reported that AsIII is more mobile in the environment, because it is more weakly bound to mineral surfaces, compared with AsV (74, 174-176).

The mobility of chromium is highly dependent on its oxidation state and pH (116). Hexavalent chromium is much more soluble than trivalent chromium. As previously stated, most research has assessed CrIII and reported that lower amounts are leached with near-neutral pH, but shows a leachability plateau from pH 8 to 12. Dubikova et al. (2006) also reported slightly higher mobility for alkaline ash and increasing releases with increasing pH (177).

In experiments reported by the USGS, two fly ash samples were placed in small volumes of oxic and anoxic freshwater (pH =7) and measured over time. Arsenic dissolved into the freshwater under both oxic and anoxic conditions and increased over time. At the end of the experiment, concentrations were above the EPA Maximum Contaminant Level (10 ppb) for total As. In the same experiment, it was observed that Cr dissolved from one fly ash sample in oxic freshwater only. Chromium did not dissolve from the second sample of fly ash. Researchers reported that Cr was probably present at insoluble species. During the study time, Cr concentrations were below the EPA Maximum Contaminant Level (100 ppb) (79).

Although Cd is located on the surface of fly ash particles, it is not very mobile in neutral or alkaline conditions, and only somewhat soluble in acidic conditions. Researchers have shown that despite the fact that Cd is located on the surface of particles, concentrations leached in water rarely surpass 0.01 mg/kg in alkaline natured fly ash (63, 178, 179) while values for acidic fly ash are approximately 0.1 mg/kg at pH=4 (180, 181).

Lead is dispersed throughout the core of fly ash particles and as a result Pb is highly insoluble and virtually immobile (<1% and often <0.1%) in both acidic and alkaline-natured fly ash samples. Researchers have shown that the immobility and insolubility occurs irrespective of the pH (178, 179, 182, 183). As with other cations, acidic conditions slightly enhance Pb leaching (156). Since Pb is a cation, acidic conditions slightly improve Pb leaching (160, 163), however, the concentrations remain at very low levels. Multiple researchers have shown that among 30 samples of fly ash with pH 11-13, none of them leaches Pb levels greater than 0.6 mg/kg (45, 177-179). Researchers from the United States reported that <1 mg/kg of Pb was released from fly ash using a range of extractants and tests (182, 184).

In addition to pH, the liquid to solid ratio (L/S) is an important factor when assessing leaching behavior. A lower L/S ratio is indicative of a material with a restricted flow and a higher L/S ratio is associated with a material having a greater flow. Researchers evaluating the impact of L/S ratios on mobility report that as L/S ratio increases, concentrations of elements reduces. DaSilva et al., (2018) showed that when L/S ratio was increased from 0.5 to 10, concentrations of As, Cd, Cr, Hg, Pb, and Se decreased. The researchers stated that the elements reached their maximum leaching at L/S of 0.5 (74). Dandautiya et al.,(2018) assessed L/S ratios from 5 to 50 and reported that Zn, Iron (Fe), Cr, Pb, Se, strontium (Sr), V, titanium (Ti) , Aluminum (Al), calcium (Ca), and Mg showed maximum leachability at L/S ratio of 5. The maximum concentration of As occurred at L/S 10 (185). Zandi (2007) showed that that leaching of most elements is not based on the L/S ratio when the L/S ratios are higher than 50, which is in agreement with the work of Jones (1995) and Nathan et al., (1999) (167).

Contamination of surface and ground water with metals have been reported in several studies carried out at locations near fly ash disposal facilities (42, 72, 146, 164, 173, 186-190). In these cases, concentrations of elements have been reported to be higher than country or the World Health Organization (WHO) environmental standards. While many studies report elevated levels of metals, Dandautiya et al., (2018) assessed groundwater contaminants around a coal-fired plant in India and found that the concentrations of Zn, As, Cu, Nickel (Ni), Pb, Ca, Mg, Cd, Cr, and Mn were below the WHO standards (185).

1. Fly Ash Exposure and Human Health

Limited epidemiological studies exist that assess the relationship between exposure to fly ash and human health. Some research has focused on the health impacts among coal-fired power plant workers exposed to “dust”, without directly studying fly ash exposure. In these studies, researchers measured dust levels in different locations, including where the coal was handled and where coal ash was removed. In some cases, they created job exposure levels to account for exposure. Few researchers have directly assessed exposure to fly ash on health among occupationally exposed workers. Those that did have reported increased oxidative stress, DNA damage, genotoxic damage, and decreased respiratory function.

Research addressing the direct exposure to fly ash on communities does not exist. Most research investigates the impact of coal-fired power plants and health in communities by utilizing distance from the coal-fired power plant as a proxy for fly ash exposure. This section highlights some of the limited epidemiological research conducted among coal-fired power plant workers, workers directly exposed to fly ash or other CCPs, and community findings.

1. *Health Outcomes Among Coal-Fired Power Plant Workers*

Few researchers have assessed cancer morbidity and mortality (191-193), markers of oxidative stress (194), and immunological profiles (195) in employees of coal-fired power plants.

Forastiere (1989) determined that there was a slight excess in total cancer mortality among 406 workers employed in two power plants in Italy. This excess was mainly due to the increased respiratory cancer that was not statistically significant. However, when assessing lung cancer, researchers determined that the observed number of lung cancer cases was greater than the expected number of cases. Although the standard mortality ratio (SMR) was increased (SMR=178), it was not statistically significant as the confidence intervals contained the null (90% Confidence Intervals = 88-321). However, the SMR, was significantly elevated for lung cancer in workers <60 years old, Furthermore, the SMRs were increased when length of exposure and latency period from first employment exceeded 10 years (192). These results were similar to findings from two other epidemiological studies of workers and lung cancer (196, 197). However, the sample size in all three studies was small and the SMRs were not statistically significant (192).

Kaur et al. (2013) studied 200 males who were divided into four groups: coal handling workers, turbine unit workers, boiler unit workers, and city electricians. They found that

malondialdehyde (MDA) levels were increased in workers in the coal handling unit, turbine unit, and boiler unit compared to the electricians (194). MDA is a byproduct of lipid peroxidation during oxidation stress. Oxidative stress has been implicated in many diseases, including neurodegenerative diseases, such as Alzheimer’s disease (198-202), atherosclerosis and cardiovascular disease (203-207), diabetic neuropathy (208, 209), and COPD (210, 211).

Bencko et al. (1980) conducted a retrospective study of mortality from cancer among workers exposed to arsenic in coal-fired power plants. The researchers assessed cancer mortality patterns among male workers in one coal-fired power plant where high arsenic content coal was combusted (exposed group) with male workers from three coal-fired power plants where low arsenic content coal was combusted (unexposed group). The rate of mortality in the exposed group was higher than the mortality in the unexposed group (38% exposed versus 23% unexposed), but the difference was not significant. However, compared to the unexposed group, exposed workers died of cancer at shorter exposure intervals and younger age (193). In the same population, Bencko et al (1988) examined the immunological profiles of workers and reported that the exposed population had significantly higher levels of carrier proteins, ceruloplasmin, transferrin, and orosomucoid, compared with the unexposed population (195).

1. *Health Outcomes of Workers Exposed to Fly Ash and CCP*

Research assessing direct exposure to fly ash or other CCPs is limited. Recent occupational studies have found that exposure to coal ash may cause genotoxic effects and disrupt biological processes. A case-control study conducted by Celik et al (2007) investigated the genotoxic damage among workers in a coal-fired power plant compared with healthy controls. Investigators found that the mean frequencies of chromosomal aberrations (CA), sister-chromatid exchanges (SEC), micronuclei (MN), and polyploidy were all significantly elevated when compared to the controls. Compared with controls, cases had increased frequency of CA (p<0.01) and increased percentage of cells with aberrations (p<0.01) in peripheral lymphocytes. Researchers reported that the most common type of aberration in cases and controls was the chromatid break, followed by a chromosome break. In addition to increased CA in the cases, there were also significant increases in SEC (p<0.01), MN (p<0.05) and the frequency of polyploidy (p<0.01), compared with controls (212). Celik et al, 2007 further investigated the genotoxic damage with respect to exposure time and age of the workers. They found a positive correlation between years of exposure and CA (p<0.05) and MN (p<0.05), but not with SCE. Age was not correlated with genotoxic damage.

In a more recent study, Zeneli et al. (2016) examined levels of metals and oxidative stress in 70 male workers exposed to fly ash (cases) compared with 27 men (controls) residing in a rural area of Kosovo. To measure levels of oxidative stress, researchers, measured gluthatione peroxidase (GPx), superoxide dismutase (SOD), and ascorbic acid in blood. Metals were also measured in blood. Compared with controls, cases had significantly higher levels of As (p<0.02), mercury (Hg) (p<0.01), Zn (p<0.007), and Se levels (p<0.0002), but lower levels of Cu (p<0.002). The concentration of Cd in the cases was higher than in controls, but it was not statistically significant (p>0.25). Researchers reported that the concentration of Hg in the power plant workers was 4.3 times greater compared to the control group. Arsenic was 1.7 times higher in the cases compared to the controls. Zeneli et al. (2016) also found that workers had significantly lower levels of SOD (p<0.002) and GPx (p<0.001) and levels of ascorbic acid was significantly lower (p<0.0001). From their research, the authors stated that the antioxidant potential of the cases signiﬁcantly differed from the controls as manifested by signiﬁcant changes in the activity of SOD and GPx and ascorbic acid (213).

Since fly ash consists of respirable particles, it would seem that researchers would have thoroughly investigated the impact of fly ash on respiratory function; however, this is not the case (67, 214-216). Schilling et al. (1988) assessed lung function among 268 worked who were exposed to fly ash for more than ten years. They created three exposure groups (low, medium, high), based on job and years of exposure. Researchers found that those workers who were in the high exposure group had a greater prevalence of chronic cough, chronic phlegm, wheeze, chest tightness, and difficulty in breathing. Researchers highlighted that these results needed to be interpreted with caution, because of the large number of smokers and ex-smokers in the sample. To further investigate lung function and fly ash, researchers measured concentrations of fly ash exposure and performed lung function testing. Concentrations of fly ash ranged from 0.08 to 21.8 mg/m3 in the low exposed group, from 0.12 to 73.31 mg/m3 in the middle group and from 0.07 to 98.62 mg/m3 in the high exposed group (214). Researchers reported that as fly ash exposure increased, an increasing effect on several lung function tests occurred. Specifically, they reported that modest effects were shown on forced vital capacity (FVC), vital capacity (VC), forced expiratory volumes in one second (FEV1), peak flow (PF), and gas transfer (DCO) among the workers in the high exposure group (214).

In two case reports, men who were exposed to large amounts of fly ash developed lung disease. Cho et al. (1994) reported that a man unloading his truck and exposed to a large amount of fly ash developed an acute case of silicosis within two weeks of exposure (215). Interestingly, no other research has investigated silicosis in workers exposed to fly ash. In a second case report, Davidson et al., (1986) reported that a 27-year-old worker exposed to fly ash developed asthma due to his exposure at work. The man’s peak expiratory flow (PEF) was taken every 2 hours for 28 days, which got worse during work, but improved when he was not working. During an inhalation test, the man responded to exposure to fly ash, but not to the placebo (216).

1. *Community Health in Relation to Coal-Fired Power Plants*

The effect of direct exposure to fly ash or other CCP has not been studied in communities. Researchers have predominately assessed the health impacts from coal-fired power plant emissions based on proximity to plants. Other researchers assessed health conditions after a power-plant closed. In addition to particulate matter, many researchers have assessed multiple pollutants that are emitted from coal-fired power plants, such as sulfur dioxide (SO2), nitrogen dioxide (NO2), and mercury (Hg). Although there is no research on direct exposure to fly ash, there is extensive epidemiological evidence reporting that emissions from coal-ﬁred power plants deleteriously impacts the health of neighboring communities. Researchers have reported significant associations between power plant emissions and mortality, poor respiratory health, cancer (lung, larynx, bladder), skin conditions, higher urinary markers for PAHs and metals, poor birth outcomes, and neurobehavioral problems (217-232).

In a recent study, Lin et al. (2019) assessed the impact of coal-fired power plants and the burden of lung cancer. To assess the burden globally, researchers evaluated annual lung cancer incidence rates from 83 countries with coal-fired power plants by utilizing the per capita coal capacities for each country. Researchers reported that over 860,000 male and over 540,000 female lung cancer cases were attributed to power plants that used coal as the primary energy source (223). Collarile et al. (2017) investigated the risk of lung and bladder cancer in people living near a coal-oil-fired power plant. Based on tertiles of exposure to benzene, NO2, SO2, and PM10, incidence rate ratios (IRR) by sex, age, and histology were computed among 1076 incident cases of lung and 650 cases of bladder cancers. For lung cancer, no excess risk was found in men, but an excess risk was found in women aged ≥ 75 years of age in the highest tertile of exposure to benzene, NO2, SO2, and PM10. No excess risk for bladder cancer was found in men, and only women aged ≥ 75 years in the highest tertile had an excess risk for bladder cancer. A major limitation of this study, was that smoking data was not collected on the participants, which may have confounded the relationship between exposure and disease (221).

Respiratory outcomes have been well-studied. In one study on respiratory complaints and spirometric parameters, Karavus et al., 2002 compared residents who lived 5 kilometers around a coal-fired power plant to residents who lived at least 30 kilometers away from the power plant. Residents who lived closer to the power plant were significantly more likely to report chest tightness and coughing attacks lasting for more than one year, compared to the residents who lived further away (chest tightness, 46.2% versus 29.2%, p=0.001; cough, 28% versus. 20.8%, p=0.024). However, productive coughing was not found to differ among the two groups (13.3% versus. 8.4%, p=0.89). Among non-smokers, Karavus et al. found that spirometric results differed between the people residing near the power and those that lived further away. People residing closer to the power plant had lower forced expiratory volume in the first second (FEV1), forced vital capacity (FVC), and mean forced expiratory flow during the middle half of the FVC (FEF25-75%) (p<0.001 for all tests) (217).

Hagemeyer et al (2019) assessed respiratory health in adults living within four neighborhoods adjacent to a coal-fired power plant with coal ash storage facilities and compared the results to unexposed comparison population. In this cross-sectional study, the researchers found that exposed adults were statistically more likely to report cough (Adjusted Odds Ratio (AOR) = 5.30, 95% Confidence Intervals (CI) = 2.60-11), shortness of breath (AOR = 2.59, 95% CI = 1.56-4.31), hoarseness (AOR = 4.02, 95% CI = 2.45-6.60), and respiratory infections (AOR=1.82, 95% CI=1.14-2.89). Furthermore, the researchers found that the exposed population had a significantly lower mean overall respiratory health score, compared with the non-exposed population (2.82 vs. 3.87, p<0.0001) (218).

Researchers investigating the impact of coal-fired power plant emissions on children’s respiratory health have been consistent in showing its health impact. Children are considered a vulnerable population because they exhibit behaviors that will increase their risk of exposure.

Children tend to breathe through their mouths and have larger lung surface area per body weight, compared to adults. Children’s lungs do not completely develop till late teen years and developing organs like the lungs are more susceptible to toxic effects and environmental pollutants. In addition, children absorb more pollutants than adults and are more likely to retain them over time because they tend to spend more time outside. Children tend to be mouth breathers as well (not just nasal breathers) which increases their ventilation rate, thereby increasing the amount of pollutants taken up by the lungs. Undeveloped immune system could also pose health risks in children (233, 234).

Rodriquez-Villamizar et al (2018) conducted a spatial cross-sectional study to assess the association between emergency department (ED) visits for asthma and residential proximity to a coal-fired power plant and a petrochemical facility. The researchers found that children who lived with closer to the power plant were ten times more likely to be admitted to the ED for asthma, than children who lived farther away. After adjusting for age, socioeconomic status and gender, an inverse association between asthma visits and distance from the power plant was determined. Interestingly, there was no association when examining relationships with the nearby petrochemical facility (219).

Sears et al. (2017) utilized a cross-sectional epidemiological study to investigate health in children living adjacent to a coal-fired power plant with coal ash storage facilities and children living 60 miles away. Although the researchers found associations with other health conditions (ADHD and gastrointestinal problems), they found an elevated but not significant adjusted odds ratio for the prevalence of asthma (AOR = 2.52, 95% CI = 0.8-7.6) (228).

Studies on neurodevelopment in children exposed to power plant emissions are few, but indicate a relationship. Tang et al (2008) assessed the effects of prenatal exposure to coal-burning pollutants on children’s development in China and found that exposure to pollutants from power plants harmed the development of children living in the study region. The researchers concluded that the level of PAH-DNA adducts in cord blood of newborns was associated with reductions in developmental quotients in both motor and language areas. Additionally, the researchers found that in utero exposure to lead from the plant deleteriously affected social development of the children (225).

A study by Liang et al. (2010) determined that coal combusted fly ash is a dominant source of Pb exposure for children living in Shanghai (235). The researchers estimated that Pb pollution in air is caused mainly by coal combustion (50%), metallurgic dust (35%), and vehicle exhaust (15%). As previously noted, Pb is associated with many neurobehavioral heath disorders in children. Furthermore, the researchers stated that based on the Pb isotopes of the children’s blood, they believed that Pb from fly ash is much easily absorbed into the blood than lead from vehicle exhaust or metallurgic dust (235).

In a study conducted in the United States, Sears and Zierold (2017) assessed the relationship between proximity to a coal-fired power plant with coal ash storage facilities and ADHD, learning difficulties, and emotional and behavioral problems. The researchers found that children living adjacent to a coal-fired power plant had an increased prevalence of ADHD compared with unexposed children living 60 miles away (AOR=3.6, 95% CI = 1.2-10.7). The logistic regression model used to determine the odds ratio was adjusted for secondhand smoke exposure, age and gender (228).

To date there is no research on community populations directly exposed to fly ash; however, there is extensive epidemiological evidence reporting that emissions from coal-ﬁred power plants deleteriously impacts the health of neighboring communities. Research is needed to advance our understanding of the health impact of fly ash, particularly as storage continues to increase in some countries while other countries battle to maintain ash that is stored in unlined landfills and surface impoundments.

**CONCLUSION**

Fly ash, which results from the combustion of coal, is of environmental concern. Although, fly ash can be beneficially reutilized in products such as concentrate, a large percentage of it is stored in landfills and surface impoundments. Fugitive dust emissions and leaching of elements into groundwater are pathways for which human populations may be exposed to the respirable fraction of fugitive dust and the trace elements in fly ash. Unfortunately, limited research on the health impacts of fly ash exists. Longer term monitoring and direct exposure assessments of communities impacted by fly ash is needed. Although researchers have proven that many of the trace elements in fly ash, such as lead and arsenic, are harmful to human health, questions such as the concentrations to which people are exposed, duration of exposure, and the reaction of these elements synergistically need to be answered to understand the health impact of exposure to fly ash. Epidemiological and environmental research on the impact of fly ash and other CCPs is needed to further policy and regulations on storage, disposal, transportation, and clean-up.

**Author Statement**

Research Funding: Authors state no funding involved.

Conflict of Interest: Authors state no conflict of interest.

Informed Consent: Informed consent is not applicable.

Ethical Approval: The conducted research is not related to either human or animal use.

**REFERENCES**

1. International Energy Agency (IEA). Coal-Fired Power, Tracking Clean Energy Progress. Available at: <https://www.iea.org/tcep/power/coal/>
2. International Energy Agency (IEA). Beta. International. Available at: <https://www.eia.gov/beta/international/>
3. United States Energy Information Administration. Coal explained. Use of coal. Available at: <https://www.eia.gov/energyexplained/coal/use-of-coal.php>
4. United States Energy Information Administration. Frequently asked questions. What is U.S. electricity generation by energy source? Available at: https://www.eia.gov/tools/faqs/faq.php?id=427&t=3
5. United States Energy Information Administration. Today in Energy. Chinese coal-fired electricity generation expected to flatten as mix shifts to renewables. Available at: <https://www.eia.gov/todayinenergy/detail.php?id=33092>
6. Chen J, Liu G, Kang Y, Wu B, Sun R, Zhou C, et al. Coal utilization in China: environmental impacts and human health. Environ Geochem Health 2014;36(4):735-753.
7. Kumar S, Singh J, Mohapatra SK. Role of particle size in assessment of physico-chemical properties and trace elements in Indian fly ash. Waste Mang Res 2018;36(11):1016-1022.
8. Shahzad Baig K, Yousaf M. Coal fired power plants: Emissions problems and controlling techniques. J Earth Sci and Clim Change 2017;8:404. doi: 10.4172/2157-7617.1000404
9. Dwivedi A, Jain MK. Fly ash -waste management and overview: A review. Recent Research in Science and Technology 2014;6(1):30-35.
10. Carlson CL, Adriano DC. Environmental impacts of coal combustion residues. J Environ Qual 1993;22:227-247
11. Brown P, Jones T, BéruBé K. The internal microstructure and fibrous mineralogy of fly ash from coal-burning power stations. Environ Pollut 2011;159(12):3324–33.
12. Kutchko BG, Kim AG. Fly ash characterization by SEM-EDS. Fuel 2006;85:25–37
13. Harris D, Heidrich C, Feuerborn J. Global aspects on coal combustion products. Available at: <https://www.coaltrans.com/insights/article/global-aspects-on-coal-combustion-products>
14. Adriano DC, Page AL, Elseewi AA, Chang AC, Straugham I. Utilization and disposal of fly and and coal residues in terrestrial ecosystem: A review. J Environ Qual 1980; 9:333-344.
15. Vejahati F, Xu Z, Gupta R. Trace elements in coal: Associations with coal and minerals and their behavior during coal utilization—A review. Fuel 2010;89:904-911.
16. Zhang X. Management of coal combustion wastes. IEA Clean Coal Centre. Available at: <https://www.usea.org/sites/default/files/012014_Management%20of%20coal%20combustion%20wastes_ccc231.pdf>
17. Electric Power Research Institute. Technical update. Coal ash: Characteristics, management, and environmental issues. Sept 2009.
18. Bednar AJ, Averett DE, Seiter JM, Lafferty B, Jones WT, Hayes CA, et al. Characterization of metals released from coal fly ash during dredging at the Kingston ash recovery project. Chemosphere 2013;92(11):1563–70.
19. Flues M, Moraes V, Mazzilli BP. The influence of a coal-fired power plant operation on radionuclide concentrations in soil. J Environ Radioact 2002;63(3):285–94.
20. Nalbandian H. Trace element emissions from coal. IEA Clean Coal Center. Available at: https://www.usea.org/sites/default/files/092012\_Trace%20element%20emissions%20from%20coal\_ccc203.pdf
21. Sager M. Environmental aspects of trace elements in coal combustion. Toxicological and Environmental Chemistry 1999;71(1-2):159-183.
22. Schwartz GE, Hower JC, Phillips AL, Rivera N, Vengosh A, Hsu-Kim H. Ranking coal ash materials for their potential to leach arsenic and selenium: Relative imporantance of ash chemistry and site biogeochemistry. Environmental Engineering Science 2018;35(7): [doi.org/10.1089/ees.2017.0347](https://doi.org/10.1089/ees.2017.0347)
23. Jegadeesan G, Al-Abed SR, Pinto P. Influence of trace metal distribution on its leachability from coal fly ash. Fuel 2008; 87: 1887–1893.
24. Huggins FE, Senior CL, Chu P, Ladwig K, Huffman GP. Selenium and arsenic speciation in fly ash from full-scale coal-burning utility plants. Environ Sci Technolog 2007; 41(9):3284-3289.
25. el-Mogazi D, Lisk DJ, Weinstein LH. A review of physical, chemical, and biological properties of fly ash and effects on agricultural ecosystems. Sci Total Environ 1988; 1:1-37.
26. Galbreath KC, Zygarlicke CJ. Formation and chemical speciation of arsenic-,chromium-, and nickel-bearing coal combustion PM2.5. Fuel Processing Technology 2004;85:701–726.
27. Meij R, te Winkel H. The emissions of heavy metals and persistent organic pollutants from modern coal-fired power stations. Atmospheric Environmental 2007; 41:9262-9272.
28. Arditsoglou A, Petaloti Ch, Terzi E, Sofoniou M, Samara C. Size distribution of trace elements and polycyclic aromatic hyrocarbons in fly ashes generated in Greek lignite-fired power plants. Sci Total Environ 2004; 323:153-167.
29. Hatori Y, Matsuyama S, Ishii K, Terakawa A, Kikuchi Y, Fujiwara H, et al. PIXE analysis of individual particles in coal fly ash. Int J PIXE 2010; 20:57-62.
30. Patra KC, Rautray TR, Tripathy BB, Nayak P. Elemental analysis of coal and coal ash by PIXE technique. Appl Radiat Isot Data Instrum Methods Use Agric Ind Med 2012;70(4):612–6.
31. EPRI (2009) Coal ash: characteristics, management and environmental issues. EPRI report 1019022, Palo Alto, CA, USA, Electric Power Research Institute, 11 pp (Sep 2009)
32. Habib MA, Basuki T, Miyashita S, Bekelesi W, Nakashima S, Techato K, Khan R, Majlis ABK, Phoungthong K. Assessment of natural radioactivity in coals and coal combustion residues from a coal-based thermoelectric plant in Bangladesh: implications for radiological health hazards. Environ Monit Assess 2019; 19:27. doi.org/10.1007/s10661-018-7160-y.
33. Ozden B, Guler E, Vaasma T, Horvath M, Kiisk M. Enrichment of naturally occurring radionuclides and trace elements in Yatagan and Yenikoy coal-fired thermal power plants, Turkey. J Environ Radioactivity 2018;188:100-107.
34. Izquierdo M. Leaching behavior of elements from coal combustion fly ash: an overview. International Journal of Coal Geology2012; 94:54-66.
35. Tishmack JK, Burns PE. The chemistry and mineralogy of coal and coal combustion products. Energy, Waste, and the Environment: a Geochemical Perspective. Gieri, R & Stille, P (eds) 2004. Geological Society, London, Special Publications, 236, 223-246.
36. Harris D, Heidrich C, Feuerborn J. Global aspects on coal combustion products. World of Coal Ash Conference, Conference Paper, 2019.
37. EPA. Environmental Protection Agency (EPA) Final Rule: Disposal of Coal Combustion Residuals from Electric Utilities. Federal Register. 2015 Jul 2;80(127):37988–92.
38. American Coal Ash Association. (November 2018). Coal Ash Recycling Reaches Record 64 Percent Amid Shifting Production and Use Patterns. Available at: <https://www.acaa-usa.org/Portals/9/Files/PDFs/Coal-Ash-Production-and-Use-2017.pdf>
39. EPA Report to Congress: Wastes from the combustion of coal by electric utility power plants. Report no. EPA/530-SW-88-002, Washington DC, USA, Environmental Protection Agency, Office of Solid Waste, 1988 Feb; pg. 4-23.
40. Cooke N. Utilizing the UK’s vast landfilled fly ash deposits. Ash at Work 2018; I: 8-9.
41. United States Environmental Protection Agency. (2010). Hazardous and solid waste

management system; identification and listing of special wastes; disposal of coal combustion residuals from electric utilities; proposed rule (Codified at 40 CFR Parts 257, 261, 264 et al.). Fed Reg. 2010;75(118):21386

1. United States Environmental Protection Agency. (2010). Hazardous and solid waste

management system; identification and listing of special wastes; disposal of coal combustion residuals from electric utilities; proposed rule (Codified at 40 CFR Parts 257, 261, 264 et al.). Fed Reg. 2010;75(118):21311

1. Li J, Zhuang X, Querol X, Font O, Moreno N, Zhou J. Environmental geochemistry of the feed coals and their combustion by-products from two coal-fired power plants in Xinjiang Province, Northwest China. Fuel 2012; 95:446-456.
2. Chatterjee AK. Fly Ash from Thermal Power Plants in India: The Challenge of 100% Utilization. Ash at Work 2018; I:20-26.
3. Izquierdo M, Querol X. Leaching behavior of elements from coal combustion fly ash: An overview. International J Coal Geology 2012;94:54-66.
4. Stanley W, Haverland R. Global trends in coal-fueled power generation and the need for CCP imports to the Americas. Ash at Work 2018;I: 14-17.
5. Heidrich C, Feuerborn HJ, Weir A. Coal combustion products: A global perspective. World of Coal Ash, Conference Paper, 2013.
6. Li J, Zhuang X, Querol X, Font O, Moreno N. A review on the applications of coal combustion products in China. International Geology Review 2018; 60(5): 671-716.
7. Ahmaruzzaman M. A review on the utilization of fly ash. Prog Energy Combust Sci 2010; 36:327–63.
8. Lauer NE, Hower JC, Hsu-Kim H, Taggart RK, Vengosh A. Naturally occurring radioactive materials in coals and coal combustion residuals in the United States. Environmental Science & Technology2015;49(18), 11227-11233.
9. Liberda EN, Chen LC. An evaluation of the toxicological aspects and potential doses from the inhalation of coal combustion products. Journal of Air and Waste Management Association 2013;63(6), 671–80.
10. Meawad AS, Bojinova DY, Pelovski YG. An overview of metals recovery from thermal power plant solid wastes. Waste Management 2010;30(12), 2548-2559.
11. Yao Z, Ji X, Sarker P, Tang J, Ge L, Xia M, Xi Y. A comprehensive review on the applications of coal fly ash. Earth-Science Reviews 2015; 141:105-121.
12. Fisher GL, Prentice BA, Silbeman D, Ondov J, Biermann AH, Ragaini RC, et al. Physical and morphological studies of size-classified coal fly ash. Enviro Sci Tech 1978; 12(4):447-451.
13. Ismail KN, Hussin K, Idris MS. Physical, chemical, and mineralogical properties of fly ash. J Nuclear and Related Technology 2007; 4:47-51.
14. Jia Y, Lighty JS. Ash particulate formation form pulverized coal under oxy-fuel combustion conditions. Environmental Science and Technology 2012; 46:5214-5221.
15. Hurley JP, Schobert HH. Ash formation during pulverized subbituminous coal combustion. 1. Characterization of coals, and inorganic transformations during early stages of burnout. Energy and Fuels 1992; 6:47-58.
16. Juda-Rezler K, Kowalczyk D. Size distribution and trace elements contents of coal fly ash from pulverized boilers. Pol. J. Environ. Stud2013; 22(1):25-40.
17. Bhatt A, Priyadarshini S, Mohanakrishnan AA, Abri A, Sattler M, Techapaphawit S. Physical, chemical, and geotechnical properties of coal fly ash: A global review. Case Studies in Construction Materials 2019; 11: e00263. [doi.org/10.1016/j.cscm.2019.e00263](https://doi.org/10.1016/j.cscm.2019.e00263).
18. Gollakota ARK, Volli V, Shu CM. Progressive utilization prospects of coal fly ash: A review. Sci Total Environ 2019; 672:951-989.
19. Bhanarkar AD, Gavane AG, Tajne DS, Tamhane SM, Nema P. Composition and size distribution of particules emissions from a coal-fired power plant in India. Fuel 2008; 87(10-11):2095-2101.
20. He Y, Luo Q, Hu H. Situation analysis and countermeasures of China’s fly ash pollution prevention and control. Procedia Environmental Sciences 2012;16, 690–696.
21. Medina A, Gamero P, Querol X, Moreno N, De León B, Almanza M, et al. Fly ash from a Mexican mineral coal I: Mineralogical and chemical characterization. Journal Haz Mat 2010; 181: 82-90.
22. Surabhi. Fly ash in India: Generation vis-à-vis utilization and Global perspective. International Journal of Applied Chemistry 2017;13(1):29-52.
23. American Coal Ash Association. 2018 coal combustion product (CCP) production & use survey report. Available at: <https://www.acaa-usa.org/Portals/9/Files/PDFs/2018-Survey-Results.pdf>
24. Jambhulkar HP, Montaha S, Shaikh S, Kumar MS. Fly ash toxicity, emerging issues and possible implications for its exploitation in agriculture; Indian scenario: A review. Chemosphere 2018; 213: 333-344.
25. Borm PJA. Toxicity and occupational health hazards of coal fly ash (CFA). A review of data and comparison to coal mine dust. Ann Occup Hyg 1997;41(6):659-676.
26. Mokhtar MM, Taib RM, Hassim MH. Understanding selected trace elements behavior in a coal-fired power plant in Malaysia for assessment of abated technologies. J Air Waste Mang Assoc 2014; 64(8):867-878.
27. Bhattacharyya S, Donahoe RJ, Patel D. Experimental study of chemical treatment of coal fly ash to reduce the mobility of priority trace elements. Fuel 2009; 88:1173-1184.
28. Spencer LLS, Drake LD. Hydrogeology of an alkaline fly ash landfill in Eastern Iowa. Groundwater 1987; 25(5):519-526.
29. Bhangare RC, Ajmal PY, Sahu SK, Pandit GG, Puranik VD. Distributions of trace elements in coal and combustion residues from five thermal power plants in India. International Journal of Coal Geology 2011;86: 349-356.
30. Verma C, Madan S, Hussain A. Heavy metal contamination of groundwater due to fly ash disposal of coal-fired thermal power plant, Parichha Jhansi, India. Cogent Engineering 2016; (3)1: 1179243. [doi.org/10.1080/23311916.2016.1179243](https://doi.org/10.1080/23311916.2016.1179243).
31. Tiruta-Barna L, Rakotoarisoa Z, Mehu J. Assessment of the multi-scale leaching behaviour of compacted coal fly ash. J Hazard Mater 2006; B137: 1466-1478.
32. [da Silva EB](https://www.ncbi.nlm.nih.gov/pubmed/?term=da%20Silva%20EB%5BAuthor%5D&cauthor=true&cauthor_uid=28768222), [Li S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Li%20S%5BAuthor%5D&cauthor=true&cauthor_uid=28768222), [de Oliveira LM](https://www.ncbi.nlm.nih.gov/pubmed/?term=de%20Oliveira%20LM%5BAuthor%5D&cauthor=true&cauthor_uid=28768222), [Gress J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Gress%20J%5BAuthor%5D&cauthor=true&cauthor_uid=28768222), [Dong X](https://www.ncbi.nlm.nih.gov/pubmed/?term=Dong%20X%5BAuthor%5D&cauthor=true&cauthor_uid=28768222), [Wilkie AC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wilkie%20AC%5BAuthor%5D&cauthor=true&cauthor_uid=28768222), et al. Metal leachability from coal combustion residuals under different pHs and liquid/solid ratios. J Hazard Mater 2018; 341:66-74.
33. [Reddy MS](https://www.ncbi.nlm.nih.gov/pubmed/?term=Reddy%20MS%5BAuthor%5D&cauthor=true&cauthor_uid=15916850), [Basha S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Basha%20S%5BAuthor%5D&cauthor=true&cauthor_uid=15916850), [Joshi HV](https://www.ncbi.nlm.nih.gov/pubmed/?term=Joshi%20HV%5BAuthor%5D&cauthor=true&cauthor_uid=15916850), [Jha B](https://www.ncbi.nlm.nih.gov/pubmed/?term=Jha%20B%5BAuthor%5D&cauthor=true&cauthor_uid=15916850). Evaluation of the emission characteristics of trace metals from coal and fuel oil fired power plants and their fate during combustion. J Hazard Mater 2005;123(1-3):242-249.
34. Chan PC, Huff J. Arsenic carcinogenesis in animals and in humans: Mechanistic, experimental, and epidemiological evidence. J Environ Sci Health 1997;C15: 83-122.
35. Hong YS, Song KH, Chung JY. Health effects of chronic arsenic exposure. J Prev Med Public Health 2014;47(5):245–252.
36. Smedley PL, Kinniburgh DG. A review of the source, behaviour and distribution of arsenic in natural waters. Applied Geochemistry 2002;17(5):517-568.
37. Deonarine A , Kolker A, and Doughten M. Trace elements in coal ash: U.S. Geological Survey Fact Sheet 2015–3037. Accessed at: <https://pubs.usgs.gov/fs/2015/3037/>
38. Huggins PE, Senior CL, Chu P, Ladwig K, Huffman GP. Selenium and arsenic speciation in fly ash from full scale coal burning utility plants. Environ Sci Technol 2007; 41:3284-3290.
39. IARC. International Agency For Research On Cancer (IARC) Monographs on the Evaluation of Carcinogenic Risks to Humans. 2018; Available at: <https://monographs.iarc.fr/wp-content/uploads/2018/06/mono100C-6.pdf>
40. Wang C-H, Hsiao CK, Chen C-L, Hsu L-I, Chiou H-Y, Chen S-Y, et al. A review of the epidemiologic literature on the role of environmental arsenic exposure and cardiovascular diseases. Toxicol Appl Pharmacol 2007;222(3):315–326.
41. [Kuo CC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kuo%20CC%5BAuthor%5D&cauthor=true&cauthor_uid=28796632), [Moon KA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Moon%20KA%5BAuthor%5D&cauthor=true&cauthor_uid=28796632), [Wang SL](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wang%20SL%5BAuthor%5D&cauthor=true&cauthor_uid=28796632), [Silbergeld E](https://www.ncbi.nlm.nih.gov/pubmed/?term=Silbergeld%20E%5BAuthor%5D&cauthor=true&cauthor_uid=28796632), [Navas-Acien A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Navas-Acien%20A%5BAuthor%5D&cauthor=true&cauthor_uid=28796632). The association of arsenic metabolism with cancer, cardiovascular disease, and diabetes: A systematic review of the epidemiological evidence. Environ Health Perspect 2017; 125(8):087001. doi: 10.1289/EHP577.
42. [Moon KA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Moon%20KA%5BAuthor%5D&cauthor=true&cauthor_uid=29040626), [Oberoi S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Oberoi%20S%5BAuthor%5D&cauthor=true&cauthor_uid=29040626), [Barchowsky A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Barchowsky%20A%5BAuthor%5D&cauthor=true&cauthor_uid=29040626), [Chen Y](https://www.ncbi.nlm.nih.gov/pubmed/?term=Chen%20Y%5BAuthor%5D&cauthor=true&cauthor_uid=29040626), [Guallar E](https://www.ncbi.nlm.nih.gov/pubmed/?term=Guallar%20E%5BAuthor%5D&cauthor=true&cauthor_uid=29040626), [Nachman KE](https://www.ncbi.nlm.nih.gov/pubmed/?term=Nachman%20KE%5BAuthor%5D&cauthor=true&cauthor_uid=29040626), et al. A dose-response meta-analysis of chronic arsenic exposure and incident cardiovascular disease. In J Epidemiol 2017; 46(6):1924-1939.
43. [James KA](https://www.ncbi.nlm.nih.gov/pubmed/?term=James%20KA%5BAuthor%5D&cauthor=true&cauthor_uid=25350952), [Byers T](https://www.ncbi.nlm.nih.gov/pubmed/?term=Byers%20T%5BAuthor%5D&cauthor=true&cauthor_uid=25350952), [Hokanson JE](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hokanson%20JE%5BAuthor%5D&cauthor=true&cauthor_uid=25350952), [Meliker JR](https://www.ncbi.nlm.nih.gov/pubmed/?term=Meliker%20JR%5BAuthor%5D&cauthor=true&cauthor_uid=25350952), [Zerbe GO](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zerbe%20GO%5BAuthor%5D&cauthor=true&cauthor_uid=25350952), [Marshall JA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Marshall%20JA%5BAuthor%5D&cauthor=true&cauthor_uid=25350952). Association between lifetime exposure to inorganic arsenic in drinking water and coronary heart disease in Colorado residents. Environ Health Perspect 2015; 123(2):128-134.
44. Coronado-González JA, Del Razo LM, García-Vargas G, Sanmiguel-Salazar F, Escobedo-de la Peña J. Inorganic arsenic exposure and type 2 diabetes mellitus in Mexico. Environ Res 2007 Jul;104(3):383–389.
45. [James KA](https://www.ncbi.nlm.nih.gov/pubmed/?term=James%20KA%5BAuthor%5D&cauthor=true&cauthor_uid=23507312), [Marshall JA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Marshall%20JA%5BAuthor%5D&cauthor=true&cauthor_uid=23507312), [Hokanson JE](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hokanson%20JE%5BAuthor%5D&cauthor=true&cauthor_uid=23507312), [Meliker JR](https://www.ncbi.nlm.nih.gov/pubmed/?term=Meliker%20JR%5BAuthor%5D&cauthor=true&cauthor_uid=23507312), [Zerbe GO](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zerbe%20GO%5BAuthor%5D&cauthor=true&cauthor_uid=23507312), [Byers TE](https://www.ncbi.nlm.nih.gov/pubmed/?term=Byers%20TE%5BAuthor%5D&cauthor=true&cauthor_uid=23507312). A case-cohort study examining lifetime exposure to inorganic arsenic in drinking water and diabetes mellitus. Environ Res 2013; 123:33-38.
46. [Grau-Perez M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Grau-Perez%20M%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), [Kuo CC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kuo%20CC%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), [Gribble MO](https://www.ncbi.nlm.nih.gov/pubmed/?term=Gribble%20MO%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), [Balakrishnan P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Balakrishnan%20P%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), [Jones Spratlen M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Jones%20Spratlen%20M%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), [Vaidya D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Vaidya%20D%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), [Francesconi KA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Francesconi%20KA%5BAuthor%5D&cauthor=true&cauthor_uid=29373862), et al. Association of low-moderate arsenic exposure and arsenic metabolism with incident diabetes and insulin resistance in the Strong Heart Family Study. Environ Health Perspect 2017; 125(12):127004. doi: 10.1289/EHP2566
47. Wang W, Xie A, Lin Y, Zhang D. Association of inorganic arsenic exposure with type 2 diabetes mellitus: a meta-analysis. J Epidmiol Community Health 2014; 68(2):176-184.
48. von Ehrenstein OS, Poddar S, Yuan Y, Mazumder DG, Eskenazi B, Basu A, et al. Children’s intellectual function in relation to arsenic exposure. Epidemiol Camb Mass 2007;18(1):44–51.
49. [Rodríguez-Barranco M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rodr%C3%ADguez-Barranco%20M%5BAuthor%5D&cauthor=true&cauthor_uid=25682472), [Gil F](https://www.ncbi.nlm.nih.gov/pubmed/?term=Gil%20F%5BAuthor%5D&cauthor=true&cauthor_uid=25682472), [Hernández AF](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hern%C3%A1ndez%20AF%5BAuthor%5D&cauthor=true&cauthor_uid=25682472), [Alguacil J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Alguacil%20J%5BAuthor%5D&cauthor=true&cauthor_uid=25682472), [Lorca A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lorca%20A%5BAuthor%5D&cauthor=true&cauthor_uid=25682472), [Mendoza R](https://www.ncbi.nlm.nih.gov/pubmed/?term=Mendoza%20R%5BAuthor%5D&cauthor=true&cauthor_uid=25682472), et al. Postnatal arsenic exposure and attention impairment in school children. Cortex 2016; 74:370-382.
50. [Rosado JL](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rosado%20JL%5BAuthor%5D&cauthor=true&cauthor_uid=17805430), [Ronquillo D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Ronquillo%20D%5BAuthor%5D&cauthor=true&cauthor_uid=17805430), [Kordas K](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kordas%20K%5BAuthor%5D&cauthor=true&cauthor_uid=17805430), [Rojas O](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rojas%20O%5BAuthor%5D&cauthor=true&cauthor_uid=17805430), [Alatorre J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Alatorre%20J%5BAuthor%5D&cauthor=true&cauthor_uid=17805430), [Lopez P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lopez%20P%5BAuthor%5D&cauthor=true&cauthor_uid=17805430), et al. Arsenic exposure and cognitive performance in Mexican schoolchildren. Environ Health Perspect 2007; 115(9):1371-1375.
51. Ramsey K. 13 - Arsenic and Respiratory Disease. In: Flora SJS, editor. Handbook of Arsenic Toxicology p. 335–347. Available at: https://www.sciencedirect.com/science/article/pii/B9780124186880000137
52. George CM, Brooks WA, Graziano JH, Nonyane BAS, Hossain L, Goswami D, et al. Arsenic exposure is associated with pediatric pneumonia in rural Bangladesh: a case control study. Environ Health 2015;14:83.
53. [Sanchez TR](https://www.ncbi.nlm.nih.gov/pubmed/?term=Sanchez%20TR%5BAuthor%5D&cauthor=true&cauthor_uid=26891939), [Perzanowski M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Perzanowski%20M%5BAuthor%5D&cauthor=true&cauthor_uid=26891939), [Graziano JH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Graziano%20JH%5BAuthor%5D&cauthor=true&cauthor_uid=26891939). Inorganic arsenic and respiratory health, from early life exposure to sex-specific effects: A systematic review. Environ Res 2016;147:537-555.
54. [Dauphiné DC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Dauphin%C3%A9%20DC%5BAuthor%5D&cauthor=true&cauthor_uid=20972800), [Ferreccio C](https://www.ncbi.nlm.nih.gov/pubmed/?term=Ferreccio%20C%5BAuthor%5D&cauthor=true&cauthor_uid=20972800), [Guntur S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Guntur%20S%5BAuthor%5D&cauthor=true&cauthor_uid=20972800), [Yuan Y](https://www.ncbi.nlm.nih.gov/pubmed/?term=Yuan%20Y%5BAuthor%5D&cauthor=true&cauthor_uid=20972800), [Hammond SK](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hammond%20SK%5BAuthor%5D&cauthor=true&cauthor_uid=20972800), [Balmes J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Balmes%20J%5BAuthor%5D&cauthor=true&cauthor_uid=20972800), et al. Lung function in adults following in utero and childhood exposure to arsenic in drinking water: preliminary findings. Int Arch Occup Environ Health 2011;84(6):591-600.
55. Li C, Wu H, Wang X, Chu Z, Li Y, Guo J. Determination of lead elemental concentration and isotopic ratios in coal ash and coal fly ash reference materials using isotope dilution thermal ionization mass spectrometry. Int J Environ Res Public Health 2019; 16, 4772; doi:10.3390/ijerph16234772.
56. Makowska D, Strugala A, Wieronska F, Bacior M. Assessment of the content, occurrence, and leachability of arsenic, lead, and thallium in wastes from coal cleaning processes. Environ Sci Pollut Res Int 2019; 26(9), 8418-8428.
57. Swanson SM, Engle MA, Ruppert LF, Affolter RH, Jones KB. Partitioning of selected trace elements in coal combustion products from two coal-burning power plants in the United States. Int J Coal Geology 2013; 113, 116-126.

100) Sandeep P, Sahu SK, Kothail P, Pandit GG. Leaching behavior of selected trace and toxic metals in coal fly ash samples collected from two thermal power plants, India. Bull Environ Contam Toxicol 2016; 97:425-431.

101) Usmani Z, Kumar V. Characterization, portioning, and potential ecological risk quantification of trace elements in coal fly ash. Environ Sci Pollut Res 2017;24:15546-15566.

102) Akar G, Polat M, Galecki G, Ipekoglu U. Leaching behavior of selected trace elements in coal fly ash samples from Yenikoy coal-fired power plants. Fuel Processing Technology 2012; 104:50-56.

103) Franus W, Wiatros-Motyka MM, Wdowin M. Coal fly ash as a resource for rare earth elements. Environmental Science and Pollution Research 2015; 22(12):9464-9474.

104) Hong S-B, Im M-H, Kim J-W, Park E-J, Shin M-S, Kim B-N, et al. Environmental lead exposure and attention deficit/hyperactivity disorder symptom domains in a community sample of South Korean school-age children. Environ Health Perspect 2015; 123(3):271–276.

105) Liu J, Liu X, Wang W, McCauley L, Pinto-Martin J, Wang Y, et al. Blood Lead Levels and children’s Behavioral and Emotional Problems: A Cohort Study. JAMA Pediatr 2014; 168(8):737–745.

106) Bellinger DC. Very low lead exposures and children’s neurodevelopment. Curr Opin Pediatr 2008;20(2):172-177.

107) [Dietrich KN](https://www.ncbi.nlm.nih.gov/pubmed/?term=Dietrich%20KN%5BAuthor%5D&cauthor=true&cauthor_uid=7678702), [Berger OG](https://www.ncbi.nlm.nih.gov/pubmed/?term=Berger%20OG%5BAuthor%5D&cauthor=true&cauthor_uid=7678702), [Succop PA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Succop%20PA%5BAuthor%5D&cauthor=true&cauthor_uid=7678702). Lead exposure and the motor developmental status of urban six-year old children in the Cincinnati Prospective Study. Pediatrics 1993; 91(2): 301-307.

108) [Rodrigues](https://ehjournal.biomedcentral.com/articles/10.1186/s12940-016-0127-y#auth-1) EM, Bellinger DC, Valeri L, Hasan, M, Quamruzzaman Q, Golam M, et al. Neurodevelopmental outcomes among 2- to 3-year-old children in Bangladesh with elevated blood lead and exposure to arsenic and manganese in drinking water.Environ Health 2016; 15: 44. doi:10.1186/s12940-016-0127-y.

109) Canfield RL, Henderson CR, Cory-Skechta DA, Cox C, Jusko TA, Lanphear BP. Intellectual impairment in children with blood lead concentrations below 10 microg per deciliter. N Engl J Med 2003; 348:1517–1526.

110) Park SK, Elmarsafawy S, Mukherjee B, Spiro A, Vokonas PS, Nie H, et al. Cumulative Lead Exposure and Age-related Hearing Loss: The VA Normative Aging Study. Hear Res 2010; 269(12):48–55.

111) Vaziri ND. Mechanisms of lead-induced hypertension and cardiovascular disease. Am J Physiol Heart Circ Physiol 2008;295(2):H454-465.

112) [Spivey](https://www.ncbi.nlm.nih.gov/pubmed/?term=Spivey%20A%5BAuthor%5D&cauthor=true&cauthor_uid=17366809) A. The weight of lead: Effects add up in adults. Environ Health Perspect 2007;115(1):A30-A36.

113) Lanphear BP, Rauch S, Auinger P, Allen RA, Hornung RW. Low-level lead exposure and mortality in US adults: a population-based cohort study. Lancet Public Health 2018; 3: e177–84.

114) Mansouri MT, Munoz-Fambuena I, Caul O. Cognitive impairment associated with chronic lead exposure in adults. Neurology, Psychiatry, and Brain Research 2018; 30:5-8.

115) IARC. International Agency For Research On Cancer (IARC) Monographs on the Evaluation of Carcinogenic Risks to Humans. Volume 87, Inorganic and Organic Lead Compounds. 2006; Available at: <https://monographs.iarc.fr/wp-content/uploads/2018/06/mono87.pdf>.

116) Huggins FE, Huffman GP. How do lithophile elements occur in organic association in bituminous coals? International Journal of Coal Geology 2004; 58: 193-204.

117) Zhitkovich A. Chromium in drinking water: sources, metabolism, and cancer risks. Chem. Res. Toxicol 2011; 24(10): 1617-1629.

118) Goodarzi F, Huggins FE, Sanei H. 2008. Assessment of elements, speciation of As, Cr, Ni and emitted Hg for a Canadian power plant burning bituminous coal. International Journal of Coal Geology 2008;74:1-12

119) Huggins FE, Shah N, Huffman GP, Kolker A, Crowley S, Palmer CA, et al. Mode of occurrence of chromium in four US coals. Fuel Processing Technology 2000; 63: 7992.

120) Ruppert L, Finkelman R, Boti E, Milosavljevic M, Tewalt S, Simon N, et al. Origin and significance of high nickel and chromium concentrations in pliocene lignite of the Kosovo Basin, Serbia. International Journal of Coal Geology 1996; 29:235-258.

121) Huggins FE, Najih M, Huffman GP. Direct speciation of chromium in coal combustion by-products by X-ray absorption fine-structure spectroscopy. Fuel 1999; 78: 233-242.

122) IARC. International Agency For Research On Cancer (IARC) Monographs on the Evaluation of Carcinogenic Risks to Humans Chromium VI Compounds. Available at: <https://monographs.iarc.fr/wp-content/uploads/2018/06/mono100C-9.pdf>.

123) Welling R, Beaumont JJ, Petersen SJ, Alexeeff GV, Steinmaus C. Chromium VI and stomach cancer: a meta-analysis of the current epidemiological evidence Occupational and Environmental Medicine 2015;72:151-159.

124) [Gatto NM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Gatto%20NM%5BAuthor%5D&cauthor=true&cauthor_uid=20430714), [Kelsh MA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kelsh%20MA%5BAuthor%5D&cauthor=true&cauthor_uid=20430714), [Mai DH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Mai%20DH%5BAuthor%5D&cauthor=true&cauthor_uid=20430714), [Suh M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Suh%20M%5BAuthor%5D&cauthor=true&cauthor_uid=20430714), [Proctor DM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Proctor%20DM%5BAuthor%5D&cauthor=true&cauthor_uid=20430714). Occupational exposure to hexavalent chromium and cancers of the gastrointestinal tract: a meta-analysis. Cancer Epidemiol 2010; 34(4): 388-399.

125) [Deng Y](https://www.ncbi.nlm.nih.gov/pubmed/?term=Deng%20Y%5BAuthor%5D&cauthor=true&cauthor_uid=30778374), [Wang M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wang%20M%5BAuthor%5D&cauthor=true&cauthor_uid=30778374), [Tian T](https://www.ncbi.nlm.nih.gov/pubmed/?term=Tian%20T%5BAuthor%5D&cauthor=true&cauthor_uid=30778374), [Lin S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lin%20S%5BAuthor%5D&cauthor=true&cauthor_uid=30778374), [Xu P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Xu%20P%5BAuthor%5D&cauthor=true&cauthor_uid=30778374), [Zhou L](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zhou%20L%5BAuthor%5D&cauthor=true&cauthor_uid=30778374), et al. The Effect of Hexavalent Chromium on the Incidence and Mortality of Human Cancers: A Meta-Analysis Based on Published Epidemiological Cohort Studies. Front Oncol 2019; 9:24. doi: 10.3389/fonc.2019.00024.

126) Gambelunghe A, Piccinini R, Ambrogi M et al. Primary DNA damage in chrome-plating workers. Toxicology 2003; 188: 187–195.

127) Wu FY, Wu WY, Kuo HW et al. Effect of genotoxic exposure to chromium among electroplating workers in Taiwan. Sci Total Environ 2001; 279: 21–28.

128) Vaglenov A, Nosko M, Georgieva R et al. Genotoxicity and radioresistance in electroplating workers exposed to chromium. Mutat Res 1999; 446: 23–34.

129) Benova D, Hadjidekova V, Hristova R et al. Cytogenetic effects of hexavalent chromium in Bulgarian chromium platers. Mutat Res 2002; 514: 29–38.

130) Bernhoft RA. Cadmium toxicity and treatment. The Scientific World Journal 2013:394652. <http://dx.doi.org/10.1155/2013/394652>.

131) IARC. International Agency For Research On Cancer (IARC) Monographs on the Evaluation of Carcinogenic Risks to Humans. Cadmium and cadmium compounds. 2006; Available at: <https://monographs.iarc.fr/wp-content/uploads/2018/06/mono100C-8.pdf>.

132) Caciari T, Sancini A, Fioravanti M, Capozzella A, Casale T, Montuori L, et al. Cadmium and

hypertension in exposed workers: A meta-analysis. Int J Occup Med Environ Health 2013;

26(3):440–456.

133) Hartwig A. Cadmium and cancer. Met Ions Life Sci 2013;11:491–507.

134) James KA, Meliker JR. Environmental cadmium exposure and osteoporosis: a review. Int J Public Health 2013;58(5):737–745.

135) Jarup L, Akesson A. Current status of cadmium as an environmental health problem. Toxicol Appl Pharmacol 2009;238(3):201-208.

136) [Wu Q](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wu%20Q%5BAuthor%5D&cauthor=true&cauthor_uid=19937228), [Magnus JH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Magnus%20JH%5BAuthor%5D&cauthor=true&cauthor_uid=19937228), [Hentz JG](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hentz%20JG%5BAuthor%5D&cauthor=true&cauthor_uid=19937228). Urinary cadmium, osteopenia, and osteoporosis in the US population. Osteoporos Int 2010; 21(8):1449-1454.

137) [Lv Y](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lv%20Y%5BAuthor%5D&cauthor=true&cauthor_uid=28407309), [Wang P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wang%20P%5BAuthor%5D&cauthor=true&cauthor_uid=28407309), [Huang R](https://www.ncbi.nlm.nih.gov/pubmed/?term=Huang%20R%5BAuthor%5D&cauthor=true&cauthor_uid=28407309), [Liang X](https://www.ncbi.nlm.nih.gov/pubmed/?term=Liang%20X%5BAuthor%5D&cauthor=true&cauthor_uid=28407309), [Wang P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wang%20P%5BAuthor%5D&cauthor=true&cauthor_uid=28407309), [Tan J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Tan%20J%5BAuthor%5D&cauthor=true&cauthor_uid=28407309), et al. Cadmium exposure and osteoporosis: A population-based study and benchmark dose estimation in Southern China. J Bone Miner Res 2017; 32(10):1990-2000.

138) Tchounwou PB, Yedjou CG, Patlolla AK, Sutton DJ. Heavy Metals Toxicity and the Environment. EXS 2012;101:133–64.

139) Davidson PW, Myers GJ, Weiss B. Mercury exposure and child development outcomes. Pediatrics 2004; 113(3), 1023-1029.

140) Tchounwou PB, Ayensu WK, Ninashvili N, Sutton D. Environmental exposure to mercury and its toxicopathologic implications for public health. Environ Toxicol 2003;18(3):149–75.

141) Grandjean P, Weihe P, White RF, Debes F, Araki S, Yokoyama K, et al. Cognitive deficit in 7-year-old children with prenatal exposure to methylmercury. Neurotoxicol Teratol 1997;19 :417– 428.

142) [Lam HS](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lam%20HS%5BAuthor%5D&cauthor=true&cauthor_uid=23416249), [Kwok KM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kwok%20KM%5BAuthor%5D&cauthor=true&cauthor_uid=23416249), [Chan PH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Chan%20PH%5BAuthor%5D&cauthor=true&cauthor_uid=23416249), [So HK](https://www.ncbi.nlm.nih.gov/pubmed/?term=So%20HK%5BAuthor%5D&cauthor=true&cauthor_uid=23416249), [Li AM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Li%20AM%5BAuthor%5D&cauthor=true&cauthor_uid=23416249), [Ng PC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Ng%20PC%5BAuthor%5D&cauthor=true&cauthor_uid=23416249), [et](https://www.ncbi.nlm.nih.gov/pubmed/?term=Fok%20TF%5BAuthor%5D&cauthor=true&cauthor_uid=23416249) al. Long term neurocognitive impact of low dose prenatal methylmercury exposure in Hong Kong. Environ Int 2013; 54:59-64.

143) [Orenstein ST](https://www.ncbi.nlm.nih.gov/pubmed/?term=Orenstein%20ST%5BAuthor%5D&cauthor=true&cauthor_uid=25062363), [Thurston SW](https://www.ncbi.nlm.nih.gov/pubmed/?term=Thurston%20SW%5BAuthor%5D&cauthor=true&cauthor_uid=25062363), [Bellinger DC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Bellinger%20DC%5BAuthor%5D&cauthor=true&cauthor_uid=25062363), [Schwartz JD](https://www.ncbi.nlm.nih.gov/pubmed/?term=Schwartz%20JD%5BAuthor%5D&cauthor=true&cauthor_uid=25062363), [Amarasiriwardena CJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Amarasiriwardena%20CJ%5BAuthor%5D&cauthor=true&cauthor_uid=25062363), [Altshul LM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Altshul%20LM%5BAuthor%5D&cauthor=true&cauthor_uid=25062363), [et](https://www.ncbi.nlm.nih.gov/pubmed/?term=Korrick%20SA%5BAuthor%5D&cauthor=true&cauthor_uid=25062363) al. Prenatal organochlorine and methylmercury exposure and memory and learning in school-age children in communities near the New Bedford Harbor Superfund site, Massachusetts. Environ Health Perspect 2014;122(11):1253-1259.

144) Smith JG, Baker TF, Murphy CA, Jett RT. Spatial and temporal trends in contaminant concentrations in Hexagenia nymphs following a coal ash spill at the Tennessee Valley Authority’s Kingston Fossil Plant. Environ Toxicol Chem 2016; 35(5):1159–71.

145) Deonarine A, Bartov G, Johnson TM, Ruhl L, Vengosh A, Hsu-Kim H. Environmental impacts of the Tennessee Valley Authority Kingston coal ash spill. 2. Effect of coal ash on methylmercury in historically contaminated river sediments. Environ Sci Technol 2013; 47(4):2100–2108.

146) Ruhl L, Vengosh A, Dwyer GS, Hsu-Kim H, Deonarine A. Environmental impacts of the

coal ash spill in Kingston, Tennessee: an 18-month survey. Environ Sci Technol 2010; 44(24):9272–9278.

147) Kumar S, Singh J, Mohapatra SK. Role of particle size in assessment of physico-chemical

properties and trace elements of Indian fly ash. Waste Management & Research 2018;

36(11): 1016 –1022.

148) Bian Z, Dong J, Lei S, Leng H, Mu S, Wang, H. The impact of disposal and treatment of coal

mining wastes on environment and farmland. Environmental Geology 2009;58(3): 625–634.

149) Cao D, Selic E, Herbell JD. Utilization of Fly Ash from Coal-fired Power Plants in China.

Journal of Zhejiang University: Science A 2008; 9: 681–687.

150) Ma SH, Xu MD, Qiqige X, Zhou, X. Challenges and Developments in the Utilization of Fly

Ash in China. International Journal of Environmental Science and Development 2017; 8:781–785.

151) Ailun Y, Kang R, Zhao X, Huang X, Zhou H, Su M. et al. The True Cost of Coal:

An Investigation into Coal Ash in China. 2010. Accessed at:

[https://www.greenpeace.org/eastasia/Global/eastasia/publications/reports/climate-energy/2010/the](https://www.greenpeace.org/eastasia/Global/eastasia/publications/reports/climate-energy/2010/thetrue-cost-of-coal-investigation-into-coal-ash-in-china.pdf)

[true-cost-of-coal-investigation-into-coal-ash-in-china.pdf](https://www.greenpeace.org/eastasia/Global/eastasia/publications/reports/climate-energy/2010/thetrue-cost-of-coal-investigation-into-coal-ash-in-china.pdf)

152) Bourdrel T, Bind MA, Bejot Y, Morel O, Argacha JF. Cardiovascular effects of air pollution. Arch Cardiovasc Dis 2017; 110(11), 634-642.

153) Stockfelt L, Andersson EM, Molnar P, Gidhagan L, Segersson D, Rosengren A, et al. Long-term effects of total and source-specific particulate air pollution on incident cardiovascular disease in Gothenburg, Sweden. Environ Res 2017; 158, 61-71.

154) Sicard P, Khaniabadi YO, Perez S, Gualtieri M, De Marco A. Effect of O3, PM10 and PM2.5 on cardiovascular and respiratory diseases in cities of France, Iran, and Italy. Environ Sci Pollut Res Int 2019; 26(31), 32645-32665.

155) Lu P, Zhang Y, Lin J, Xia G, Zhang W, Knibbs LD et al. Multi-city study on air pollution and hospital outpatient visits for asthma in China. Environ Pollut 2020; 257, 113638. doi: 10.1016/j.envpolt.2019.113638.

156) Block ML, Calderon-Garciduenas L. Air pollution: mechanisms of neuroinflammation and

CNS disease. Trends Neurosci 2009;32(9):506-516.

157) Calderon-Garciduenas L, Franco-Lira M, Torres-Jardon R, Henriquez-Roldan C, Barragan-

Mejia G, Valencia-Salazar G, et al. Pediatric respiratory and systemic effects of chronic air

pollution exposure: nose, lung, heart, and brain pathology. Toxicol Pathol 2007;35(1):154-162.

158) Iyer R.The surface chemistry of leaching coal fly ash. J Haz Mat 2002;

93: 321-329.

159) Kukier U, Ishak CF, Sumner ME, Miller WP. Composition and element solubility of

magnetic and non-magnetic fly ash fractions. Environmental Pollution 2003; 123: 255-266.

160) Jones DR. The leaching of major and trace elements from coal ash. In: Swaine, DJ,

Goodarzi, F. (Eds), Environmental Aspects of Trace Elements in Coal, Springer, 1995.

161) Baba A, Kaya A. Leaching characteristics of fly ash from thermal power plants of Soma and

Tuncbilek, Turkey. Environ Monit Assess 2004; 91(1-3):171-181.

162) [Komonweeraket K](https://www.ncbi.nlm.nih.gov/pubmed/?term=Komonweeraket%20K%5BAuthor%5D&cauthor=true&cauthor_uid=25555664), Cetin B, [Benson CH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Benson%20CH%5BAuthor%5D&cauthor=true&cauthor_uid=25555664), [Aydilek AH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Aydilek%20AH%5BAuthor%5D&cauthor=true&cauthor_uid=25555664), [Edil TB](https://www.ncbi.nlm.nih.gov/pubmed/?term=Edil%20TB%5BAuthor%5D&cauthor=true&cauthor_uid=25555664). Leaching characteristics of toxic constituents from coal fly ash mixed soils under the influence of pH. Waste Manag 2015;38:174-184.

163) Singh RK, Gupta NC, Guha BK. pH dependence leaching characteristics of selected metals from coal fly ash and its impact on groundwater quality. International Journal of Chemical and Environmental Engineering 2014;5: 218–222.

# 164) Wang J. Statistical study on distribution of multiple dissolved elements and a water quality assessment around a simulated stackable fly ash. [Ecotoxicology and Environmental Safety](https://www-sciencedirect-com.ezproxy3.lhl.uab.edu/science/journal/01476513) 2018, 159: 46-50.

165) Wang J, Ban H, Teng X, Wang H, Ladwig K. Impacts of pH and ammonia on the leaching of Cu(II) and Cd(II) from coal fly ash. Chemosphere 2006; 64:1892-1898.

166) Su T, Wang J. Modeling batch leaching behavior of arsenic and selenium from bituminous coal fly ashes. Chemosphere 2011;85: 1368-1374.

167) Zandi M, Russel NV. Design of a Leaching test framework for coal fly ash accounting or environmental conditions. Environ Monit Assess 2007;131: 509-526.

168) Tiwari MK, Bajpai S, Dewangan UK, Tamrakar RK. Assessment of heavy metal concentrations in surface water sources in an industrial region of central India. Karbala Int J Mod Sci 2015; 1:9–14.

169) Jankowskia J, Warda CR, French D, Groves S. Mobility of trace elements from selected Australian fly ashes and its potential impact on aquatic ecosystems. Fuel 2006;85: 243-256.

170) Flues M, Sato IM, Scapin MA, Cotrim MEB, Camargo IMC. Toxic elements mobility in coal and ashes of Figueira coal power plant, Brazil. Fuel 2013; 103:430-4:36.

171) GoodarziF, Huggins, FE, SaneiH. Assessment of elements, speciation of As, Cr, Ni and emitted Hg for a Canadian power plant burning bituminous coal. International Journal of Coal Geology 2008;74(1):1-12.

172) van der Hoek, EE, Bonouvrie PA, Comans RNJ. Sorption of As and Se on mineral components of fly ash: Relevance for leaching processes. Applied Geochemistry 1994;9:403-412.

173) Kapoor S, Christian RA Transport of toxic elements through leaching in and around ash disposal sites. Int J Environ Sci Dev 2016;7(1):65–68.

174) Manning BA, Goldberg S. Adsorption and stability of arsenic (III) at the clay mineral-water interface. Environ Sci Technol 1997; 31: 2005-2011.

175) Manning BA. Goldberg S. Aresinc (III) and arsenic (V) adsorption on three California soils. Soil Sci 1997; 162: 886-895.

176) Goldberg S. Competitive adsorption of arsenate and arsenite on oxides and clay minerals. Soil Sci Soc. Am. J 2002;66: 413-421.

177) Dubikova, M., Jankowski, J., Ward, C.R., French, D. Modelling element mobility in water fly ash interactions. Co-operative Research Centre for Coal in Sustainable Development, Research Report 61, 2016. Accessed at: <http://pandora.nla.gov.au/pan/64389/200808281328/www.ccsd.biz/publications/635.html>

178) Moreno N, Querol X, Andrés JM, Stanton K, Towler M, Nugteren H, et al. Physico-chemical characteristics of European pulverized coal combustion fly ashes. Fuel 2005; 84:1351-1363.

179) Nathan Y, Dvorachek M, Pelly I, Mimran U. Characterization of coal fly ash from Israel. Fuel 1999;78, 205-213.

180) Jankowski J, Ward CR, French D. Preliminary assessment of trace element mobilisation from Australian fly ashes. Co-operative Research Centre for Coal in Sustainable Development, Research Report 2004, 45, Accessed at: <http://pandora.nla.gov.au/pan/64389/200808281328/www.ccsd.biz/publications/425.html>.

181) Ward CR, French D, Jankowski J, Dubikova M, Li Z, Riley KW. Element mobility from fresh and long-stored acidic fly ashes associated with an Australian power station. International Journal of Coal Geology 2009; 80: 224-236.

182) Kim AG, Kazonich G, Dahlberg M. Relative solubility of cations in class F fly ash: Environmental Science and Technology 2003;37: 4507-4511.

183) Praharaj T, Powell MA, Hart BR, Tripathy S. Leachability of elements from subbituminous coal fly ash from India. Environmental International 2002; 27:609-615.

184) Kim AG, Hesbach P. Comparison of fly ash leaching methods. Fuel 2009; 88: 926-937.

185) Dandautiya R, Singh AP, Kundu S. Impact assessment of fly ash on ground water quality: An experimental study using batch leaching tests. Waste Management & Research 2018; 36(7): 624-634.

186) Singh RK, Gupta NC, Guha BK. Assessment of ground water contamination for heavy metals in the proximity of ash ponds. Elixir Pollut 2014; 75:28016–28019.

187) Ruhl L, Vengosh A, Dwyer GS, Hsu-Kim H, Schwartz G, Romanski A, et al. The impact of coal combustion residue effluent on water resources: A North Carolina example. Environmental Science & Technology 2012; 46(21):12226‒12233.

188) Nyale SM, Eze CP, Akinyeye RO, et al. The leaching behaviour and geochemical fractionation of trace elements in hydraulically disposed weathered coal fly ash. J Environ Sci Health A Tox Hazard Subst Environ Engl 2014; 49(2):233-242.

189) Ruhl L, Vengosh A, Dwyer GS, Hsu-Kim H, Deonarine A. Environmental Impacts of the Coal Ash Spill in Kingston, Tennessee: An 18-Month Survey.Environ. Sci. Technol 2010; 44(24): 9272-9278.

190) Ruhl L, Vengosh A, Dwyer GS, Hsu-Kim H, Deonarine A, Bergin M, Kravchenko J. Survey of the Potential Environmental and Health Impacts in the Immediate Aftermath of the Coal Ash Spill in Kingston, Tennessee.Environ. Sci. Technol 2009; 43(16): 6326-6333.

191) Nichols L, Sorahan T. Mortality of UK electricity generation and transmission workers, 1973-2002. Occupational Medicine 2002; 55:541-548.

192) Forastiere F, Pupp N, Magliola E, Valesini S, Tidei F, Perucci CA. Respiratory cancer mortality among worker employed in thermoelectric power plants. Scand J Work Environ Health 1989; 15(6):383-386.

193) Bencko V, Symon K, Stalnik L, Batora J, Vanco E, Svandova E. Rate of malignant tumor mortality among coal burning power plant workers occupationally exposed to arsenic. J Hyg Epidemiol Microbiol Immunol 1980; 24(3): 278-284.

194) Kaur S, Gill MS, Gupta K, Manchanda K. Effect of occupation on lipid peroxidation and antioxidant status in coal-fired thermal plant workers. Int J Appl Basic Med Res 2013; 3(2):93-97.

195) Bencko V, Wagner V, Wagnerova M, Batora J. Immunological profiles in workers of a power plant burning coal rich in arsenic content. J Hyg Epidemiol Microbiol Immunol 1988; 32(2):137-46.

196) Camarrano A, Crosignani P, Berrino F, Berra A. Additional follow-up of cancer mortality among workers in a thermoelectric power plant [Letter to the editor]. Scand J Work Environ Health 1986; 12:631-632.

197) Petrelli A, Menniti-Ippolito F, Taroni F, Raschetti R, Magarotto G. A retrospective cohort mortality study of workers of two thermoelectric power plants: fourteen-year follow-up results. Eur J Epidemiol 1989; 5:87- 89.

198) Chen Z, Zhong C. Oxidative stress in Alzheimer’s disease. Neurosci Bull 2014; 30(2):271-281.

199) Tonnies E, Trushina E. Oxidative stress, synaptic dysfunction, and Alzheimer’s disease. J Alzheimers Dis 2017; 57(4): 1105-1121.

200) [Birnbaum JH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Birnbaum%20JH%5BAuthor%5D&cauthor=true&cauthor_uid=29414602), [Wanner D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wanner%20D%5BAuthor%5D&cauthor=true&cauthor_uid=29414602), [Gietl AF](https://www.ncbi.nlm.nih.gov/pubmed/?term=Gietl%20AF%5BAuthor%5D&cauthor=true&cauthor_uid=29414602), [Saake A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Saake%20A%5BAuthor%5D&cauthor=true&cauthor_uid=29414602), [Kündig TM](https://www.ncbi.nlm.nih.gov/pubmed/?term=K%C3%BCndig%20TM%5BAuthor%5D&cauthor=true&cauthor_uid=29414602), [Hock C](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hock%20C%5BAuthor%5D&cauthor=true&cauthor_uid=29414602), et al. Oxidative stress and altered mitochondrial protein expression in the absence of amyloid-β and tau pathology in iPSC-derived neurons from sporadic Alzheimer’s disease patients. Stem Cell Res 2018; 27:121-130.

201) [Rekatsina M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rekatsina%20M%5BAuthor%5D&cauthor=true&cauthor_uid=31782132), [Paladini A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Paladini%20A%5BAuthor%5D&cauthor=true&cauthor_uid=31782132), [Piroli A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Piroli%20A%5BAuthor%5D&cauthor=true&cauthor_uid=31782132), [Zis P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zis%20P%5BAuthor%5D&cauthor=true&cauthor_uid=31782132), [Pergolizzi JV](https://www.ncbi.nlm.nih.gov/pubmed/?term=Pergolizzi%20JV%5BAuthor%5D&cauthor=true&cauthor_uid=31782132), [Varrassi G](https://www.ncbi.nlm.nih.gov/pubmed/?term=Varrassi%20G%5BAuthor%5D&cauthor=true&cauthor_uid=31782132). Pathophysiology and Therapeutic Perspectives of Oxidative Stress and Neurodegenerative Diseases: A Narrative Review. Adv Ther 2019. doi: 10.1007/s12325-019-01148-5.

202) [Singh A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Singh%20A%5BAuthor%5D&cauthor=true&cauthor_uid=31013638), [Kukreti R](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kukreti%20R%5BAuthor%5D&cauthor=true&cauthor_uid=31013638), [Saso L](https://www.ncbi.nlm.nih.gov/pubmed/?term=Saso%20L%5BAuthor%5D&cauthor=true&cauthor_uid=31013638), [Kukreti S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kukreti%20S%5BAuthor%5D&cauthor=true&cauthor_uid=31013638). Oxidative stress: A key modulator in neurodegernative diseases. Molecules 2019;24(8): E1583. doi: 10.3390/molecules24081583.

203) [Kattoor AJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kattoor%20AJ%5BAuthor%5D&cauthor=true&cauthor_uid=28921056), [Pothineni NVK](https://www.ncbi.nlm.nih.gov/pubmed/?term=Pothineni%20NVK%5BAuthor%5D&cauthor=true&cauthor_uid=28921056), [Palagiri D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Palagiri%20D%5BAuthor%5D&cauthor=true&cauthor_uid=28921056), [Mehta JL](https://www.ncbi.nlm.nih.gov/pubmed/?term=Mehta%20JL%5BAuthor%5D&cauthor=true&cauthor_uid=28921056). Oxidative Stress in Atherosclerosis. [Curr Atheroscler Rep](https://www.ncbi.nlm.nih.gov/pubmed/28921056) 2017; 19(11):42. doi: 10.1007/s11883-017-0678-6.

204) [Senoner T](https://www.ncbi.nlm.nih.gov/pubmed/?term=Senoner%20T%5BAuthor%5D&cauthor=true&cauthor_uid=31487802), [Dichtl W](https://www.ncbi.nlm.nih.gov/pubmed/?term=Dichtl%20W%5BAuthor%5D&cauthor=true&cauthor_uid=31487802). Oxidative Stress in Cardiovascular Diseases: Still a Therapeutic Target? [Nutrients](https://www.ncbi.nlm.nih.gov/pubmed/31487802) 2019; 11(9). pii: E2090. doi: 10.3390/nu11092090.

205) [Fiorentino TV](https://www.ncbi.nlm.nih.gov/pubmed/?term=Fiorentino%20TV%5BAuthor%5D&cauthor=true&cauthor_uid=23448484), [Prioletta A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Prioletta%20A%5BAuthor%5D&cauthor=true&cauthor_uid=23448484), [Zuo P](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zuo%20P%5BAuthor%5D&cauthor=true&cauthor_uid=23448484), [Folli F](https://www.ncbi.nlm.nih.gov/pubmed/?term=Folli%20F%5BAuthor%5D&cauthor=true&cauthor_uid=23448484). Hyperglycemia-induced oxidative stress and its role in diabetes mellitus related cardiovascular diseases. [Curr Pharm Des](https://www.ncbi.nlm.nih.gov/pubmed/23448484) 2013;19(32):5695-703.

206) [Faria A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Faria%20A%5BAuthor%5D&cauthor=true&cauthor_uid=27916650), [Persaud SJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Persaud%20SJ%5BAuthor%5D&cauthor=true&cauthor_uid=27916650). Cardiac oxidative stress in diabetes: Mechanisms and therapeutic potential. [Pharmacol Ther](https://www.ncbi.nlm.nih.gov/pubmed/27916650) 2017; 172:50-62.

(207) [Brown DI](https://www.ncbi.nlm.nih.gov/pubmed/?term=Brown%20DI%5BAuthor%5D&cauthor=true&cauthor_uid=25634975), [Griendling KK](https://www.ncbi.nlm.nih.gov/pubmed/?term=Griendling%20KK%5BAuthor%5D&cauthor=true&cauthor_uid=25634975) . Regulation of signal transduction by reactive oxygen species in the cardiovascular system. [Circ Res](https://www.ncbi.nlm.nih.gov/pubmed/25634975) 2015; 116(3):531-49.

208) [Babizhayev MA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Babizhayev%20MA%5BAuthor%5D&cauthor=true&cauthor_uid=25427889), [Strokov IA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Strokov%20IA%5BAuthor%5D&cauthor=true&cauthor_uid=25427889), [Nosikov VV](https://www.ncbi.nlm.nih.gov/pubmed/?term=Nosikov%20VV%5BAuthor%5D&cauthor=true&cauthor_uid=25427889), [Savel'yeva EL](https://www.ncbi.nlm.nih.gov/pubmed/?term=Savel'yeva%20EL%5BAuthor%5D&cauthor=true&cauthor_uid=25427889), [Sitnikov VF](https://www.ncbi.nlm.nih.gov/pubmed/?term=Sitnikov%20VF%5BAuthor%5D&cauthor=true&cauthor_uid=25427889), [Yegorov YE](https://www.ncbi.nlm.nih.gov/pubmed/?term=Yegorov%20YE%5BAuthor%5D&cauthor=true&cauthor_uid=25427889), et al. The Role of Oxidative Stress in Diabetic Neuropathy: Generation of Free Radical Species in the Glycation Reaction and Gene Polymorphisms Encoding Antioxidant Enzymes to Genetic Susceptibility to Diabetic Neuropathy in Population of Type I Diabetic Patients. [Cell Biochem Biophys](https://www.ncbi.nlm.nih.gov/pubmed/25427889) 2015; 71(3):1425-43.

209) [Hosseini A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hosseini%20A%5BAuthor%5D&cauthor=true&cauthor_uid=23738033), [Abdollahi M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Abdollahi%20M%5BAuthor%5D&cauthor=true&cauthor_uid=23738033). Diabetic neuropathy and oxidative stress: therapeutic perspectives. [Oxid Med Cell Longev](https://www.ncbi.nlm.nih.gov/pubmed/23738033) 2013;168039. doi: 10.1155/2013/168039.

210) [Magallón M](https://www.ncbi.nlm.nih.gov/pubmed/?term=Magall%C3%B3n%20M%5BAuthor%5D&cauthor=true&cauthor_uid=31766150), [Navarro-García MM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Navarro-Garc%C3%ADa%20MM%5BAuthor%5D&cauthor=true&cauthor_uid=31766150), [Dasí F](https://www.ncbi.nlm.nih.gov/pubmed/?term=Das%C3%AD%20F%5BAuthor%5D&cauthor=true&cauthor_uid=31766150). Oxidative Stress in COPD. [J Clin Med](https://www.ncbi.nlm.nih.gov/pubmed/31766150) 2019; 8(11): E1953. doi: 10.3390/jcm8111953.

211) [Kirkham PA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Kirkham%20PA%5BAuthor%5D&cauthor=true&cauthor_uid=23880677), [Barnes PJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Barnes%20PJ%5BAuthor%5D&cauthor=true&cauthor_uid=23880677). Oxidative stress in COPD. [Chest](https://www.ncbi.nlm.nih.gov/pubmed/23880677) 2013; 144(1):266-273.

212) Celik M, Donbak L, Unal F, Yuzbasioglu D, Aksoy H, Yilmaz S. Cytogenetic damage in workers from a coal-fired power plant. Mutat Res 2007;627(2):158-163.

213) Zeneli L, Sekovanic A, Aivazi-Leonard M, Kurti-Nexhat D. Alterations in antioxidant defense system of workers chronically exposed to arsenic, cadmium and mercury from coal flying ash. Environ Geochem Health 2016; 38:65–72.

214) Schilling CJ, Tams IP, Schilling RS, Nevitt A, Rossiter CE, Wilkinson B. A survey into the respiratory effects of prolonged exposure to pulverised fuel ash. British Journal of Industrial Medicine 1988; 45: 810-817.

215) Cho K, Cho YJ, Shrivastava DK, Kapre SS. Acute lung disease after exposure to fly ash. Chest 1994; 106(1):309–11.

216) Davison AG, Durham S, Taylor JN. Asthma caused by pulverized fuel ash. British Medical Journal 1986; 292(6535): 1561.

217) Karavus M, Aker A, Cebeci D, Tasdemir M, Bayram N, Cali S. Respiratory complaints and spirometric parameters of the villagers living around the Seyitomer coal-fired thermal power plant in Kütahya, Turkey. Ecotoxicol Environ Saf 2002; 52(3):214-220.

218) Hagemeyer AN, Sears CG, Zierold KM. Respiratory health in adults residing near a coal-burning power plant with coal ash storage facilities: A cross-sectional epidemiological study. Int J Environ Res Public Health 2019; 16(19):3642. doi: [10.3390/ijerph16193642](https://dx.doi.org/10.3390%2Fijerph16193642).

219) [Rodriguez-Villamizar LA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rodriguez-Villamizar%20LA%5BAuthor%5D&cauthor=true&cauthor_uid=29356659), [Rosychuk RJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rosychuk%20RJ%5BAuthor%5D&cauthor=true&cauthor_uid=29356659), [Osornio-Vargas A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Osornio-Vargas%20A%5BAuthor%5D&cauthor=true&cauthor_uid=29356659), [Villeneuve PJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Villeneuve%20PJ%5BAuthor%5D&cauthor=true&cauthor_uid=29356659), [Rowe BH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rowe%20BH%5BAuthor%5D&cauthor=true&cauthor_uid=29356659). Proximity to two main sources of industrial outdoor air pollution and emergency department visits for childhood asthma in Edmonton, Canada. [Can J Public Health](https://www.ncbi.nlm.nih.gov/pubmed/?term=proximity+to+two+main+sources+of+industrial+outdoor+air+pollution+and+emergency+department+visits+for+childhood+asthma) 2018; 108(5-6):e523-e529. doi: 10.17269/cjph.108.6136.

220) Zierold KM, Sears CG, Hagemeyer AN. Health symptoms among adults living near a coal-burning power plant. Arch Environ Occup Health 2019; 1-8. doi: 10.1080/19338244.2019.1633992.

221) Collarile P, Bidoli E, Barbone F, Zanier L, Del Zotto S, Fuser S, Stel F, et al. Residence in proximity of a coal-oil-fired thermal power plant and risk of lung and bladder cancer in North-Eastern Italy. A population-based study: 1995-2009. Int J Environ Res Public Health 2017; 14;860. doi:10.3390/ijerph1 4080860.

222) Garcia-Perez J, Pollan M, Boldo E, [Pérez-Gómez B](https://www.ncbi.nlm.nih.gov/pubmed/?term=P%C3%A9rez-G%C3%B3mez%20B%5BAuthor%5D&cauthor=true&cauthor_uid=19187950), [Aragonés N](https://www.ncbi.nlm.nih.gov/pubmed/?term=Aragon%C3%A9s%20N%5BAuthor%5D&cauthor=true&cauthor_uid=19187950), [Lope V](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lope%20V%5BAuthor%5D&cauthor=true&cauthor_uid=19187950), et al. Mortality due to lung, laryngeal and bladder cancer in towns lying in the vicinity of combustion installations. Sci Total Environ 2009; 407(8):2593-2602.

223) [Lin CK](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lin%20CK%5BAuthor%5D&cauthor=true&cauthor_uid=30691464), [Lin RT](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lin%20RT%5BAuthor%5D&cauthor=true&cauthor_uid=30691464), [Chen T](https://www.ncbi.nlm.nih.gov/pubmed/?term=Chen%20T%5BAuthor%5D&cauthor=true&cauthor_uid=30691464), [Zigler C](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zigler%20C%5BAuthor%5D&cauthor=true&cauthor_uid=30691464), [Wei Y](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wei%20Y%5BAuthor%5D&cauthor=true&cauthor_uid=30691464), [Christiani DC](https://www.ncbi.nlm.nih.gov/pubmed/?term=Christiani%20DC%5BAuthor%5D&cauthor=true&cauthor_uid=30691464). A global perspective on coal-fired power plants and burden of lung cancer. [Environ Health](https://www.ncbi.nlm.nih.gov/pubmed/30691464) 2019;18(1):9. doi: 10.1186/s12940-019-0448-8.

224) [Hu SW](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hu%20SW%5BAuthor%5D&cauthor=true&cauthor_uid=21803351), [Chan YJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Chan%20YJ%5BAuthor%5D&cauthor=true&cauthor_uid=21803351), [Hsu HT](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hsu%20HT%5BAuthor%5D&cauthor=true&cauthor_uid=21803351), [Wu KY](https://www.ncbi.nlm.nih.gov/pubmed/?term=Wu%20KY%5BAuthor%5D&cauthor=true&cauthor_uid=21803351), [Chang Chien GP](https://www.ncbi.nlm.nih.gov/pubmed/?term=ChangChien%20GP%5BAuthor%5D&cauthor=true&cauthor_uid=21803351), [Shie RH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Shie%20RH%5BAuthor%5D&cauthor=true&cauthor_uid=21803351), et al. Urinary levels of 1-hydroxypyrene in children residing near a coal-fired power plant. [Environ Res](https://www.ncbi.nlm.nih.gov/pubmed/21803351) 2011; 111(8):1185-1191.

225) [Tang D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Tang%20D%5BAuthor%5D&cauthor=true&cauthor_uid=18470301), [Li TY](https://www.ncbi.nlm.nih.gov/pubmed/?term=Li%20TY%5BAuthor%5D&cauthor=true&cauthor_uid=18470301), [Liu JJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Liu%20JJ%5BAuthor%5D&cauthor=true&cauthor_uid=18470301), [Zhou ZJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zhou%20ZJ%5BAuthor%5D&cauthor=true&cauthor_uid=18470301), [Yuan T](https://www.ncbi.nlm.nih.gov/pubmed/?term=Yuan%20T%5BAuthor%5D&cauthor=true&cauthor_uid=18470301), [Chen YH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Chen%20YH%5BAuthor%5D&cauthor=true&cauthor_uid=18470301), et al. Effects of prenatal exposure to coal-burning pollutants on children's development in China. [Environ Health Perspect](https://www.ncbi.nlm.nih.gov/pubmed/18470301) 2008;116(5):674-679.

226) [Tang D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Tang%20D%5BAuthor%5D&cauthor=true&cauthor_uid=24647528), [Lee J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Lee%20J%5BAuthor%5D&cauthor=true&cauthor_uid=24647528), [Muirhead L](https://www.ncbi.nlm.nih.gov/pubmed/?term=Muirhead%20L%5BAuthor%5D&cauthor=true&cauthor_uid=24647528), [Li TY](https://www.ncbi.nlm.nih.gov/pubmed/?term=Li%20TY%5BAuthor%5D&cauthor=true&cauthor_uid=24647528), [Qu L](https://www.ncbi.nlm.nih.gov/pubmed/?term=Qu%20L%5BAuthor%5D&cauthor=true&cauthor_uid=24647528), [Yu J](https://www.ncbi.nlm.nih.gov/pubmed/?term=Yu%20J%5BAuthor%5D&cauthor=true&cauthor_uid=24647528), [Perera F](https://www.ncbi.nlm.nih.gov/pubmed/?term=Perera%20F%5BAuthor%5D&cauthor=true&cauthor_uid=24647528). Molecular and neurodevelopmental benefits to children of closure of a coal burning power plant in China. [PLoS One](https://www.ncbi.nlm.nih.gov/pubmed/24647528) 2014;9(3):e91966. doi: 10.1371/journal.pone.0091966.

227) [Perera F](https://www.ncbi.nlm.nih.gov/pubmed/?term=Perera%20F%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), [Li TY](https://www.ncbi.nlm.nih.gov/pubmed/?term=Li%20TY%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), [Zhou ZJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Zhou%20ZJ%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), [Yuan T](https://www.ncbi.nlm.nih.gov/pubmed/?term=Yuan%20T%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), [Chen YH](https://www.ncbi.nlm.nih.gov/pubmed/?term=Chen%20YH%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), [Qu L](https://www.ncbi.nlm.nih.gov/pubmed/?term=Qu%20L%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), [Rauh VA](https://www.ncbi.nlm.nih.gov/pubmed/?term=Rauh%20VA%5BAuthor%5D&cauthor=true&cauthor_uid=18941584), et al. Benefits of reducing prenatal exposure to coal-burning pollutants to children's neurodevelopment in China. [Environ Health Perspect](https://www.ncbi.nlm.nih.gov/pubmed/18941584) 2008;116(10):1396-1400.

228) Sears CG, Zierold KM. Health of children living near coal ash. [Glob](https://www.ncbi.nlm.nih.gov/pubmed/28804748) Ped Health 2017; 4:2333794X17720330. doi: 10.1177/2333794X17720330.

229) Tang D, Li TY, Liu JJ, Chen YH, Qu L, Perera F. PAH-DNA adducts in cord blood and fetal and child development in a Chinese cohort. Environ Health Perspect 2006;114(8):1297-1230.

230) Chen CS, Yuan TH, Shie RH, Wu KY, Chan CC. Linking sources to early effects by profiling urine metabolome of residents living near oil refineries and coal-fired power plants. Environ Int 2017;102:87-96.

231) Markandva A, Wilkinson P. Electricity generation and health. Lancet 2007;370(9591):979-990.

232) [Gohlke JM](https://www.ncbi.nlm.nih.gov/pubmed/?term=Gohlke%20JM%5BAuthor%5D&cauthor=true&cauthor_uid=21339091), [Thomas R](https://www.ncbi.nlm.nih.gov/pubmed/?term=Thomas%20R%5BAuthor%5D&cauthor=true&cauthor_uid=21339091), [Woodward A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Woodward%20A%5BAuthor%5D&cauthor=true&cauthor_uid=21339091), [Campbell-Lendrum D](https://www.ncbi.nlm.nih.gov/pubmed/?term=Campbell-Lendrum%20D%5BAuthor%5D&cauthor=true&cauthor_uid=21339091), [Prüss-Üstün A](https://www.ncbi.nlm.nih.gov/pubmed/?term=Pr%C3%BCss-%C3%9Cst%C3%BCn%20A%5BAuthor%5D&cauthor=true&cauthor_uid=21339091), [Hales S](https://www.ncbi.nlm.nih.gov/pubmed/?term=Hales%20S%5BAuthor%5D&cauthor=true&cauthor_uid=21339091), [Portier CJ](https://www.ncbi.nlm.nih.gov/pubmed/?term=Portier%20CJ%5BAuthor%5D&cauthor=true&cauthor_uid=21339091). Estimating the global public health implications of electricity and coal consumption. Environ Health Perspect 2011;119(6):821-826.

233) Bateson TF, Schwartz J. Children’s response to air pollutants. J Toxicol Environ Health A 2008;71(3):238–243.

234) Salvi S. Health effects of ambient air pollution in children. Paediatr Respir Rev 2007; 8(4):275–80.

235) Liang F, Zhang G, Tan M, Yan C, Li X, Li Y, et al. Lead in children's blood is mainly caused by coal-fired ash after phasing out of leaded gasoline in Shanghai. Environ Sci Technol 2010;44(12):4760-4765.